For 1990-2009 cars

### Circuit Description

When you first turn ON the ignition, the inflatable restraint sensing and diagnostic and seat belt pretensioner module (SDM) performs tests to diagnose critical malfunctions within itself. Then, the SDM proceeds with the RESISTANCE MEASUREMENT test to measure the deployment loop resistances to ensure that they are within their respective normal resistance ranges.

### Conditions for Running the DTC

When the ignition voltage is within the normal operating voltage range, the SDM monitors its deployment records to determine all previous commanded deployments.

### Conditions for Setting the DTC

The DTC will set if any one of the following criteria have been met by the SDM:

• | There has been a driver or passenger frontal air bag commanded deployment.

• | There has been three pretensioner-only commanded deployments.

• | There has been three driver side air bag commanded deployments.

• | There has been three passenger side air bag commanded deployments.

### Action Taken When the DTC Sets

The SDM turns ON the AIR BAG warning lamp.

### Conditions for Clearing the DTC

This DTC is latched. This DTC will clear when the SDM is replaced.

### Diagnostic Aids

The SDM is capable of one frontal air bag deployment command, three side air bag deployment commands, and three pretensioner deployment commands. Once any one of these criteria has been met, the SDM requires replacement.

### Test Description

The numbers below refer to the step numbers on the diagnostic table:

1. This step replaces the SDM.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform A Diagnostic System Check - SIR? | -- | Go to Step 2 | Go to Diagnostic System Check - SIR
2 |

1. Turn OFF the ignition.
2. Replace the inflatable restraint sensing and diagnostic and seat belt pretenioner module (SDM). Refer to Inflatable Restraint Sensing and Diagnostic and Seat Belt Pretensioner Module Replacement .

Did you complete the replacement?

--

Go to Step 3

--

3 |

1. Reconnect all SIR components.
2. Verify that all components and connectors are properly mounted.
3. Turn ON the ignition, with the engine OFF.
4. Use the scan tool in order to clear the DTCs.

Did you complete the action?

--

Go to Diagnostic System Check - SIR

--