For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .

Important: Remove both rear seatback cushions from vehicle in order to prevent damage.

2. Remove the rear seatback cushion. Refer to Rear Seat Back Replacement .
3. Remove the inner hinges from the rear seatback. Refer to Seat Back Hinge Replacement - Rear Inner .
4. Remove the rear compartment access door from the vehicle.

Transfer the cover and the knob.

### Installation Procedure

1. Install the rear compartment access door to the vehicle.
2. Install the inner hinges to the rear seatback. Refer to Seat Back Hinge Replacement - Rear Inner .
3. Install the rear seatback cushions. Refer to Rear Seat Back Replacement .
4. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .