For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment floor carpet. Refer to Rear Floor Trim Plate Replacement .
2. Remove the jack and handle kit. Refer to Jack and Tool Stowage Container Replacement .
3. Open the cd/stowage door (3)
4. Remove the nuts retaining the cd/stowage door (3).
5. Remove the cd/stowage door (3).
6. Remove the protective edge (1) around seat back opening.
7. Remove the shock tower cover.
8. Remove the screws and push retainers.
9. Remove the RH compartment side trim.

### Installation Procedure

1. Install the RH compartment side trim.
2. Install the screws and push retainers.
3. Install the shock tower cover.
4. Install the protective edge (1) around seat back opening.
5. Install the cd/stowage door (3).
6. Install the nuts retaining the cd/stowage door (3).
7. Close the cd/stowage door (3)
8. Install the jack and handle kit. Refer to Jack and Tool Stowage Container Replacement .
9. Install the rear compartment floor carpet. Refer to Rear Floor Trim Plate Replacement .