For 1990-2009 cars

## Control Valve Body Wiring Harness

### Removal Procedure

1. Remove the oil pan and oil filter. Refer to Changing Fluid and Oil Filter .
2. Disconnect the electrical connectors from solenoid valves (1, 2).
3. Remove the wiring harness connector from transmission housing.
4. Remove the wiring harness.

### Installation Procedure

1. Install the wiring harness.
2. Install the wiring harness connector to transmission housing.
3. Connect the electrical connectors to solenoid valves (1, 2).
4. Install the oil pan and the oil filter. Refer to Changing Fluid and Oil Filter .