For 1990-2009 cars

1. Use a solvent and a stiff brush to clean the transfer case.
2. Remove the following components from the front output shaft:

• | The front output yoke nut

• | The flat washer

• | The rubber sealing washer

• | The front output yoke

3. Remove the speed sensor from the rear bearing retainer.
4. Remove the four-wheel drive indicator switch from the front case half.
5. Remove the rear bearing retainer bolts from the rear case half.
6. Remove the rear bearing retainer from the rear case half.