For 1990-2009 cars

### Removal Procedure

1. Remove the rear fascia. Refer to Rear Bumper Fascia Replacement in Bumpers.
2. Open the rear compartment lid.
3. Open the rear compartment passenger side panel.
4. Remove the rear quarter relief valve:

• | Push in the clips.

• | Remove the valve through the exterior of the vehicle.

### Installation Procedure

1. Install the rear quarter relief valve:

• | Install the valve with the rubber flaps facing downward in order to prevent water intrusion.

• | Inspect that the tabs are fully seated.

2. Close the rear compartment passenger side panel.
3. Close the rear compartment lid.
4. Install the rear fascia. Refer to Rear Bumper Fascia Replacement in Bumpers.