For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Wiper/Washer System Check performed? | -- | Go to Step 2 | Go to Wiper/Washer System Check
2 |

1. Disconnect the windshield wiper motor connector.
2. Turn the ignition switch to the ON position.
3. Turn the windshield wiper/washer switch to the LOW position.
4. Use a DMM in order to measure the voltage between terminal A of the windshield wiper motor connector and ground.

Does the voltage measure at the specified value?

B+

Go to Step 4

Go to Step 3

3 |

1. Locate an open or a high resistance in CKT B7.
2. Repair the open or the high resistance in CKT B7.
3. If CKT B7 is OK, replace the windshield wiper/washer switch. Refer to Windshield Wiper and Washer Switch Replacement - On Vehicle in Steering.

Is the repair complete?

--

Go to Step 5

--

4 |

1. Check for a faulty connection at terminal A of the windshield wiper motor connector.
2. If the connection is OK, replace the windshield wiper motor. Refer to Windshield Wiper Motor Replacement .

Is the repair complete?

--

Go to Step 5

--

5 |

1. Reconnect all of the connectors and the components that were disconnected.
2. Verify that the windshield wipers operate properly at LOW speed.

Do the windshield wipers operate properly at LOW speed?

--

Go to Wiper/Washer System Check

Go to Step 1