For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system, if equipped with the Inflatable Restraint Side Impact System. Refer to Disabling the SIR System in Restraints.
2. Remove front door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the speaker grille. Refer to Speaker Grille Replacement .
4. Remove the trim panel pocket screws.
5. Unhook the tabs in the corners of the trim panel pocket.
6. Remove the pocket.

### Installation Procedure

1. Install the pocket while hooking the corner tabs.
2. Install the pocket screws.
3. Install the speaker grille. Refer to Speaker Grille Replacement .
4. Install front door trim panel. Refer to Front Side Door Trim Panel Replacement .
5. Enable the SIR system, if equipped with the Inflatable Restraint Side Impact System. Refer to Enabling the SIR System in Restraints.