For 1990-2009 cars

### Removal Procedure

1. Remove the glass panel. Refer to Sunroof Glass Panel Replacement .
2. Remove the headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.
3. Remove the sunroof actuator. Refer to Sunroof Actuator Replacement .
4. Remove the water gutter. Refer to Water Gutter Replacement .
5. Remove the sunscreen. To remove the suncreen, push in on the slide until they release from the tracks.

### Installation Procedure

1. Install the sunscreen. To install the sunscreen, snap in both sides to the track.
2. Install the water gutter. Refer to Water Gutter Replacement .
3. Install the sunroof actuator. Refer to Sunroof Actuator Replacement .
4. Install the headliner. Refer to in Headlining Trim Panel Replacement in Interior Trim.
5. Install the glass panel. Refer to Sunroof Glass Panel Replacement .