For 1990-2009 cars

## Drive Belt Tensioner Removal Serpentine

1. Use a wrench on the center bolt of the tensioner pulley (5) and rotate downward to release drive belt tension.
2. Remove the belt (7) from the water pump pulley.
3. Release the AIR pipe clamps (2).
4. Remove the AIR pipe bracket nut (1).
5. Remove the upper generator nut (6).
6. Remove the AIR pipe.
7. Remove the accessory drive belt.
8. Remove the belt tensioner bolts.
9. Remove the tensioner from the engine.