For 1990-2009 cars

### Removal Procedure

1. Insert a flat bladed tool under the front edge of the switch plate.
2. Gently pry upwards to release the front edge of the switch plate from the door trim panel.
3. Disconnect the power window switch electrical connector.
4. Remove the switch.

### Installation Procedure

1. Connect the power window switch electrical connector.
2. Install the power window switch by pressing down on the front and rear sides of the switch plate to engage the retainer clips into the door trim panel.