For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Seat Replacement .
2. Remove the front seatback cushion cover. Refer to Front Seat Back Cushion Cover Replacement .
3. Remove the front seatback cushion pad from the seatback frame.

### Installation Procedure

1. Install the front seatback cushion pad to the seatback frame.
2. Install the front seatback cushion cover. Refer to Front Seat Back Cushion Cover Replacement .
3. Install the front seat. Refer to Seat Replacement .