For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Remove the inner belt sealing strip. Refer to Rear Door Window Belt Inner Sealing Strip Replacement .
4. Remove the outer belt sealing strip. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .
5. Remove the door window weatherstrip. Refer to Rear Side Door Window Weatherstrip Replacement .
6. Remove the door vent window and division channel. Refer to Rear Side Door Stationary Window and Front Channel Replacement .
7. Remove the inside door handle. Refer to Rear Side Door Inside Handle Replacement .
8. Remove the door window regulator and motor. Refer to Rear Side Door Window Regulator Replacement .
9. Remove the door window. Refer to Rear Side Door Window Replacement .
10. Remove the door upper sealing strip.

### Installation Procedure

1. Install the door upper sealing strip.
2. Install the door window. Refer to Rear Side Door Window Replacement .
3. Install the door window regulator and motor. Refer to Rear Side Door Window Regulator Replacement .
4. Install inside door handle. Refer to Rear Side Door Inside Handle Replacement .
5. Install the door vent window division channel. Refer to Rear Side Door Stationary Window and Front Channel Replacement .
6. Install the door window weatherstrip. Refer to Rear Side Door Window Weatherstrip Replacement .
7. Install the outer belt sealing strip. Refer to Rear Door Window Belt Outer Sealing Strip Replacement .
8. Install the inner belt sealing strip. Refer to Rear Door Window Belt Inner Sealing Strip Replacement .
9. Install the water deflector. Refer to Rear Side Door Water Deflector Replacement .
10. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .