For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Position (APP) Sensor Mounting Bolts | 22 N·m | 16 lb ft
AIR Check Valve | 30 N·m | 22 lb ft
Air Intake Duct Clamps | 3 N·m | 27 lb in
AIR Pipe to Manifold Bolts | 20 N·m | 15 lb ft
AIR Pump Bracket to Frame Nuts | 12 N·m | 106 lb in
AIR Pump to Bracket Bolts | 10 N·m | 89 lb in
AIR Shut-Off Valve to Bracket Screws | 4 N·m | 35 lb in
AIR Vacuum Control Valve Solenoid to Bracket Bolts | 4 N·m | 35 lb in
Camshaft Position Sensor | 8 N·m | 71 lb in
Coil Pack Retainer Bolts | 8 N·m | 71 lb in
Crankshaft Position Sensor | 8 N·m | 71 lb in
ECM Ground Wire Screw | 4 N·m | 35 lb in
ECM Mounting Nuts | 4 N·m | 35 lb in
ECT Sensor | 21 N·m | 15 lb ft
Engine Mount Bracket | 60 N·m | 44 lb ft
EVAP Canister Purge Valve Bracket | 8 N·m | 71 lb in
EVAP Service Port Retaining Nut | 4 N·m | 35 lb in
EVAP Canister Vent Valve Bolt | 10 N·m | 89 lb in
Exhaust Heat Shield Nuts | 4 N·m | 35 lb in
Fuel Pressure Regulator Clamp Bolt | 5 N·m | 44 lb in
Fuel Rail Attaching Bolts | 8 N·m | 71 lb in
Fuel Rail Bracket Bolts | 8 N·m | 71 lb in
Fuel Rail Supply and Return Lines | 15 N·m | 11 lb ft
Fuel Sender Locking Nut | 50 N·m | 37 lb ft
Fuel Tank Pressure (FTP) Sensor | 2 N·m | 18 lb in
Fuel Tank Retaining Strap | 30 N·m | 22 lb ft
Heater Hose Retainer Bracket | 8 N·m | 71 lb in
In-Line Fuel Filter Line Bolts | 25 N·m | 18 lb ft
In-Line Fuel Filter Strap Attaching Bolt | 18 N·m | 13 lb ft
Intake Air Resonator Nuts | 3 N·m | 27 lb in
Intake Plenum Switchover Solenoid to Plenum Bolts | 8 N·m | 71 lb in
Intake Plenum Switchover Valve to Plenum Bolts | 8 N·m | 71 lb in
Intake Resonance Switchover Valve Bolts | 8 N·m | 71 lb in
Knock Sensor (KS) | 20 N·m | 15 lb ft
Oil Cooler Lines at Engine Block | 30 N·m | 22 lb ft
Oxygen Sensors (O2S) | 30 N·m | 22 lb ft
Rear Frame Rail Support Bolts | 8 N·m | 71 lb in
Throttle Body Assembly Mounting Bolts | 22 N·m | 16 lb ft
Wiring Harness Channel Bolts | 8 N·m | 71 lb in