For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Automatic Transmission Shift Lock Control Solenoid | Attached to the automatic transmission control base, to the left of the shift lever | -- | --
Automatic Transmission Shift Lock Control Switch | Attached to the automatic transmission control base, to the right of the shift lever | -- | --
Automatic Transmission Shift Lock/Unlock Switch | Attached to the automatic transmission control base, to the left of the shift lever | -- | --
Body Control Module (BCM) | Mounted on the lower RH A-pillar, behind the trim panel | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Fuel Tank Filler Door Lock Release Switch | Center of the IP, to the left of the heater and A/C control | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Body Rear End Connector End Views in Body Rear End
Fuse Block | Mounted to the IP, lower LH side of the steering column | -- | --
Instrument Cluster | LH side of the IP, above the steering column | -- | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Lifting Magnet | Attached to the steering column, next to the ignition switch | -- | Engine Electrical Connector End Views in Engine Electrical
Stop Lamp Switch | Attached to the brake pedal | -- | Lighting Systems Connector End Views in Lighting Systems
C200B | IP wiring harness to body wiring harness, at lower LH A-pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C205 | IP wiring harness to automatic transmission control switches, attached to the automatic transmission control base, to the right of the shift lever | -- | Inline Harness Connector End Views in Wiring Systems
G103 | Body and IP wiring harness, located at the LH front of the engine compartment, underneath the battery tray | Wiper/Washer Component Views in Wiper/Washer System | --
P110 | Rear LH corner of the engine compartment | -- | --
S140 | IP wiring harness, near the brake fluid minimum capacity sensor connector branch break off | -- | --
S200 | IP wiring harness, approximately 15 cm (6 in) from cruise release switch and stoplamp switch branch break off, towards G201 branch break off | -- | --
S208 | /P wiring harness, on the stop lamp switch connector branch, near the break off | -- | --
S215 | IP wiring harness, approximately 18 cm (7 in) from cruise release switch and stop lamp switch branch break off, to the right of the DLC connector branch break off. | -- | --
S217 | IP wiring harness, near the multifunction relay K134 connector branch break off | -- | --
S250 | IP wiring harness, near the gauge cluster connector branch break off | -- | --
S251 | IP wiring harness, near the G201 branch break off | -- | --
S252 | IP wiring harness, near the G201 branch break off | -- | --
S277 | IP wiring harness, Attached to buss-bar on the automatic transmission shift lever base | -- | --