For 1990-2009 cars

### Removal Procedure

1. Use a plastic tool as needed in order to loosen the locking compound.
2. Carefully thread the steering wheel tilt cover out of the tilt mechanism.

### Installation Procedure

1. Coat the steering wheel tilt lever with a medium strength locking compound, GM P/N 12345862 or equivalent.
2. Install the steering wheel tilt lever until fully seated and not stripped.