For 1990-2009 cars

#### Tools Required

J 36850 Transjel®

1. Before installing the planetary carrier assembly (653), align the markings, if present, on the planetary pinion gears so that they line up with the markings on the carrier.
2. Install the planetary carrier and output shaft assembly (653).
3. Install the input sun gear washer (652).
4. Install the input sun gear bearing (651). Use J 36850 or equivalent to hold the bearing in place.