For 1990-2009 cars

### Removal Procedure

1. Remove the inflatable restraint steering wheel module coil. Refer to Steering Wheel Inflator Module Coil Replacement
2. Insert a small pointed awl or wire into the ignition lock cylinder release pin hole.
3. Pull out the ignition lock cylinder.

### Installation Procedure

1. Install the lock cylinder:

• | Look into the hole that receives the lock cylinder on the lower RH side in order to locate the locking lever.

• | Carefully push down on the locking lever using a small flat-bladed tool untill an audible click is heard.

• | Install the lock cylinder.

2. Install the inflatable restraint steering wheel module coil. Refer to Steering Wheel Inflator Module Coil Replacement