For 1990-2009 cars

## Air Distributor Duct Replacement Passenger Side

### Removal Procedure

1. Remove the RH access panel.
2. Remove the outer air deflector screw.
3. Remove the outer air deflector.

### Installation Procedure

1. Install the outer air deflector.
2. Install the outer air deflector screw until fully seated and not stripped.
3. Install the RH access panel.

## Air Distributor Duct Replacement Drivers Side

### Removal Procedure

1. Remove the LH outer air deflector.
2. Remove the dash panel air deflector screw.
3. Remove the dash panel air deflector.

### Installation Procedure

1. Install the dash panel air deflector.
2. Install the dash panel air deflector screw until fully seated and not stripped.
3. Install the LH outer air deflector, angle the channels (1) on the deflector to install.