For 1990-2009 cars

Caution: Exposure to isocyanates during paint preparation and application processes can cause severe breathing problems. Read and follow all of the instructions from the manufacturers of painting materials, equipment, and protective gear.

1. Wash with detergent and water.
2. Clean with solvent.
3. Repair and feather edge damaged area.
4. Apply a self-etching primer and allow to dry.
5. Apply a primer-surfacer and allow to dry.
6. Sand basecoat paint area with recommended grit paper. (For clearcoat only, wet sand with ultra-fine or finer paper or hand compound.)
7. Clean with solvent and tack wipe.
8. Apply topcoat.