For 1990-2009 cars

### Removal Procedure

1. Remove the rear heated seat switch panel from the front floor console rear vent housing by gently prying the side tabs.
2. Remove the connector from the lighter.
3. Remove the cigar lighter from the panel.

### Installation Procedure

1. Install the cigar lighter to the panel.
2. Install the connector to the lighter.
3. Install the rear heated seat switch panel to the front floor console rear vent housing.