For 1990-2009 cars

#### Transmission General Specifications (4L30-E)

Name | Hydra-matic 4L30-E
--- | ---
RPO Codes | ML4
Production Location | Strasbourg, France
Vehicle Platform (Engine/Transmission) Usage | V
Transmission Drive | Longitudinally Mounted Rear Wheel Drive
1st Gear Ratio | 2.86:1
2nd Gear Ratio | 1.62:1
3rd Gear Ratio | 1.00:1
4th Gear Ratio | 0.72:1
Reverse | 2.00:1
Torque Converter Size (Turbine Diameter) | 245 mm
Pressure Taps | Line Pressure
Transmission Fluid Type | DEXRON® III
Transmission Type: 4 | Four Forward Gears
Transmission Type: L | Longitudinal Mount
Transmission Type: 30 | Torque Capacity Series
Transmission Type: E | Electronic Controls
Position Quadrant | P, R, N, D, 3, 2, 1
Case Material | Die Cast Aluminum
Transmission Weight Dry (including converter) | 69.1 kg (152 lbs)
Transmission Weight Wet (including converter) | 76.0 kg (167 lbs)
Maximum Trailer Towing Capacity | 454 kg (1,000 lbs)
Maximum Gross Vehicle Weight (GVW) | 3,500 kg (7,716 lbs)