For 1990-2009 cars

### Removal Procedure

1. Remove the front and/or rear side door sill trim plates.

Use a plastic tool to assist in lifting up on the corner to remove from door sill.

2. Remove the gasket from sill trim plates.
3. Discard old retaining clips.

### Installation Procedure

1. Install new retaining clips to the sill trim plates.
2. Install the gasket to the sill trim plates.
3. Install the front and/or rear side door sill trim plates by snapping into place.