For 1990-2009 cars

### Removal Procedure

1. Remove the rear panel to the heated seat switch from the rear vent housing of the front floor console by gently prying the side tabs.
2. Remove the connector from the lighter.
3. Remove the cigar lighter from the panel.

### Installation Procedure

1. Install the cigar lighter to panel.
2. Install the connector to lighter.
3. Install the rear panel to the heated seat switch to the rear vent housing of the front floor console.