For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Seat Belt Schematics
1 | Did you review Seat Belt System Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Seat Belts
2 |

1. Turn OFF the ignition.
2. Note the SEAT BELT indicator while turning ON the ignition.

Does the SEAT BELT indicator remain OFF at all times?

Go to Step 3

Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems

3 |

1. Turn OFF the ignition.
2. Disconnect the seat belt switch connector.
3. Test the seat belt switch signal circuit for an open or a high resistance.

Did you find and correct the condition?

Go to Step 7

Go to Step 4

4 | Test the seat belt switch for an open or a high resistance. Did you find and correct the condition? | Go to Step 7 | Go to Step 5
5 | Test the seat belt switch ground circuit for an open or a high resistance. Did you find and correct the condition? | Go to Step 7 | Go to Step 6
6 | Replace the gauge cluster. Refer to Instrument Cluster Replacement in Instrument Panel, Gauges and Console. Did you complete the replacement? | Go to Step 7 | --
7 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3