For 1990-2009 cars
SIR Components
SIR Schematics
Handling ESD Sensitive Parts Notice
SIR Caution
SIR Caution
Handling ESD Sensitive Parts Notice

### Circuit Description

The inflatable restraint Sensing and Diagnostic and Seat Belt Pretensioner Module (SDM) performs tests to diagnose critical malfunctions within itself when the ignition switch is turned ON. The SDM monitors the six firing loops to detect leakage currents to ground in the frontal and side air bag inflator module and seat belt pretensioner circuits. The deployment loop resistances are measured to ensure they are within their respective normal resistance ranges. Upon passing these tests, and if the energy reserve is charged up, the firing transistors are tested. The SDM service wait time is 1 minute. Refer to On-Vehicle Service for enable/disable procedures.

### Conditions for Setting the DTC

1. Neither of the two side air bag circuits is open.
2. The ignition is within normal operating voltage range.
3. The measured leakage currents to system voltage in the driver side air bag deployment loop are above a specified value.

DTC 86 will set once these conditions are met. This test is run during the SDM Turn-ON tests.

### Action Taken When the DTC Sets

• | The SDM sets a Diagnostic Trouble Code.

• | The SDM turns ON the AIR BAG warning lamp.

### Conditions for Clearing the DTC

Current and History DTC codes must be cleared using a scan tool Clear DTC Information command. If the circuit fault has been successfully repaired and the conditions which caused the DTC to set are no longer existing, the DTC may be cleared using the scan tool.

### Diagnostic Aids

A short circuit to a voltage source in the inflatable restraint passenger seat module circuit or a short circuit between the communication signal line of the LH or RH inflatable restraint Side Impact Sensor can set this DTC. Inspect CKTs AM13 and XM14 carefully for cutting and/or chafing. A careful inspection of the circuits and components indicated on the DTC 86 Table is essential to make sure that the replacement SDM will not be damaged.

When measurements are requested in this table, use J 39200 Digital Multimeter with the correct terminal adapter from J 35616 Connector Test Adapter Kit. When a check for proper connection is requested, refer to Intermittents and Poor Connections . When a wire, connector or terminal repair is requested, use J-38125 Terminal Repair Kit and refer to Wiring Repair .

### Test Description

The following numbers refer to the step numbers on the diagnostic table:

1. This test isolates the malfunction to one side of the inflatable restraint passenger seat module yellow 2-way integral harness connector.

2. This test isolates the malfunction to one side of the inflatable restraint passenger seat harness located under the RH front seat track cover.

3. This test determines whether the malfunction is in CKT AM13.

4. This test determines whether the malfunction is in CKT XM14.

#### DTC 86 Passenger Side Air Bag Deployment Loop Short to Voltage

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the SIR Diagnostic Check performed? | -- | Go to Step 2 | Go to SIR Diagnostic System Check
2 |

1. Turn the ignition switch OFF.
2. Wait 1 minute until the capacitors in the Sensing and Diagnostic and Seat Belt Pretensioner Module (SDM) have discharged.
3. Remove the passenger seat back cover. Refer to Seat Back Replacement - Front in Seats.
4. Disconnect the inflatable restraint passenger seat module 2-way integral connector.
5. Using the J 38715-30 adapter, connect the J 38715-A to the inflatable restraint passenger seat module 2-way integral connector.
6. Turn the ignition switch to the ON position.
7. Use the scan to request the SIR Diagnostic Trouble Codes (DTCs).

Is a current DTC 86 displayed?

--

Go to Step 4

Go to Step 3

3 | Replace the inflatable restraint passenger seat module. Refer to Inflatable Restraint Seat Module Replacement - Passenger . Is the replacement complete? | -- | Go to Step 15 | --
4 |

1. Turn the ignition switch to the OFF position.
2. Wait 1 minute until the capacitors in the Sensing and Diagnostic and Seat Belt Pretensioner Module (SDM) have discharged.
3. Disconnect the inflatable restraint passenger seat module yellow 2-way harness connector C209 located under the RH seat track cover.
4. Using the J 38715-55 adapter, connect 38715-A to the inflatable restraint passenger seat module 2-way integral connector.
5. Turn the ignition switch to the ON position.
6. Use the scan to request the SIR Diagnostic Trouble Codes (DTCs).

Is a current DTC 86 displayed?

--

Go to Step 6

Go to Step 5

5 | Replace the inflatable restraint passenger seat harness. Is the replacement complete? | -- | Go to Step 15 | --
6 |

1. Turn the ignition switch to the OFF position.
2. Disconnect the J 38715-A.
3. Disconnect the SDM. Refer to Inflatable Restraint Sensing and Diagnostic and Seat Belt Pretensioner Module Replacement .
4. Check for proper connection at terminal 13 and terminal 14 on the SDM harness connector.

Is the harness connector damaged or corroded?

--

Go to Step 7

Go to Step 9

7 | Replace the IP harness. Are the repairs complete? | -- | Go to Step 8 | --
8 | Check for proper connection at terminals 13 and 14 on the SDM. Are the terminals damaged or corroded? | -- | Go to Step 10 | Go to Step 15
9 | Check for proper connection at terminals 13 and 14 on the SDM. Are the terminals damaged or corroded? | -- | Go to Step 10 | Go to Step 11
10 | Replace the inflatable restraint Sensing and Diagnostic and Seat Belt Pretensioner Module (SDM). Refer to Inflatable Restraint Sensing and Diagnostic and Seat Belt Pretensioner Module Replacement . Are the repairs complete? | -- | Go to Step 15 | --
11 |

1. Insert J 42113 Shorting Bar Tool into the SDM harness connector terminal above terminals 13 and 14 on the SDM harness connect
2. Turn the ignition switch to the ON position.
3. Use the J 39200 to measure the voltage on the SDM harness connector from terminal 13 to terminal 7 (ground).

Is the measured voltage less than the specified value?

1 V

Go to Step 13

Go to Step 12

12 |

1. Turn the ignition switch OFF.
2. Repair the short to voltage condition in CKT AM13.

Is the repair complete?

--

Go to Step 15

--

13 | Use the J 39200 to measure the voltage on the SDM harness connector from terminal 14 to terminal 7 (ground). Is the measured voltage less than the specified value? | 1 V | Go to Integrity Check | Go to Step 14
14 |

1. Turn the ignition switch OFF.
2. Repair the short to voltage condition in CKT XM14.

Is the repair complete?

--

Go to Step 15

--

15 | Reconnect all of the SIR components, make sure all the components are properly mounted. Have all the SIR components been reconnected and properly mounted? | -- | Go to Step 16 | --
16 | Clear all the SIR DTCs. Have all the DTCs been cleared? | -- | Go to SIR Diagnostic System Check | --