For 1990-2009 cars

Table 1: | Inline Connector C100
Table 2: | Inline Connector C101
Table 3: | Inline Connector C102
Table 4: | Inline Connector C105
Table 5: | Inline Connector C106
Table 6: | Inline Connector C108
Table 7: | Inline Connector C110
Table 8: | Inline Connector C111
Table 9: | Inline Connector C112
Table 10: | Inline Connector C200A
Table 11: | Inline Connector C200B
Table 12: | Inline Connector C201
Table 13: | Inline Connector C205
Table 14: | Inline Connector C207 (With Side Airbags)
Table 15: | Inline Connector C208 (With Side Airbags)
Table 16: | Inline Connector C209 (With Side Airbags)
Table 17: | Inline Connector C210
Table 18: | Inline Connector C301
Table 19: | Inline Connector C302
Table 20: | Inline Connector C303
Table 21: | Inline Connector C304
Table 22: | Inline Connector C305
Table 23: | Inline Connector C310
Table 24: | Inline Connector C320
Table 25: | Inline Connector C400
Table 26: | Inline Connector C401
Table 27: | Inline Connector C403
Table 28: | Inline Connector C405
Table 29: | Inline Connector C500
Table 30: | Inline Connector C600

#### Inline Connector C100

Connector Part Information |

• | 12059472

• | ASM 7F M/P MIXED (BLK)

Connector Part Information

• | 12052200

• | ASM 7M M/P MIXED (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | GRY/RED | RA1 | RH Cornering Lamp Signal | A | GRY/RED | RA998 | RH Cornering Lamp Signal
B | BLK/WHT | FM1 | LH Park/Turn Lamp Signal | B | BLK/WHT | FM40 | LH Park/Turn Lamp Signal
C | BLK/GRN | FU1 | RH Park/Turn Lamp Signal | C | BLK/GRN | FU40 | RH Park/Turn Lamp Signal
D | GRY/BLK | RF1 | LH Cornering Lamp Signal | D | GRY/BLK | RF998 | LH Cornering Lamp Signal
E | BLK | F1 | Ground to G103 | E | BLK | F400 | Ground to G103
F | GRY/GRN | RU1 | B+ from Fuse #26 | F | GRY/GRN | RU40 | B+ from Fuse #26
G | BLK/BLU | FP1 | Fog Lamp On Signal | G | BLK/BLU | FP27 | Fog Lamp On Signal
H | BLU/WHT | PM4 | Outside Temperature SIgnal | H | BLU/WHT | PM4 | Outside Temperature SIgnal
J | BLU | P11 | Solar/Twilight Sensor Ground | J | BLU | P11 | Solar/Twilight Sensor Ground

#### Inline Connector C101

Connector Part Information |

• | ZFW 6-3

• | 6 WAY F (GRY)

Connector Part Information

• | ZMW 6-3

• | 6 WAY M (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RED | A990 | B+ from Fuse #33 | 1 | RED | A2 | B+ from Fuse #33
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | YEL/BLU | BP900 | A/C Cutout Signal | 3 | YEL/BLU | BP1 | A/C Cutout Signal
4 | BLK/WHT | FM7 | A/C Request Signal | 4 | BLK/WHT | FM7 | A/C Request Signal
5 | BRN | X79 | B+ from Fuse #13 | 5 | BRN | X69 | B+ from Fuse #13
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

#### Inline Connector C102

Connector Part Information |

• | ZFW 6-4

• | 6 WAY F (BRN)

Connector Part Information

• | ZMW 6-4

• | 6 WAY M (BRN)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
2 | BLU/GRN | PU1 | Oil Pressure Switch Signal | 2 | BLU/GRN | PU1 | Oil Pressure Switch Signal
3 | BLU/WHT | PM1 | Charging Indicator Signal | 3 | BLU/WHT | PM1 | Charging Indicator Signal
4 | BRN/GRN | XU4 | Oil Level Signal | 4 | BRN/GRN | XU600 | Oil Level Signal
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | BLK | F120 | Oil Level Signal | 6 | BLK | F63 | Oil Level Signal
8 | BLK/RED | FA50 | Starter Switch Signal | 8 | BLK/RED | FA501 | Starter Switch Signal
14 | BLU/YEL | PB1 | Oil Pressure Sensor Signal | 14 | BLU/YEL | PB90 | Oil Sressure Sensor Signal

#### Inline Connector C105

Connector Part Information |

• | ZFW 20-2

• | 20 WAY F (WHT)

Connector Part Information

• | ZMW 20-2

• | 20 WAY M (WHT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BRN | X61 | B+ Switch Ignition to Ignition Coils | 1 | BRN | X68 | B+ Switch Ignition to Ignition Coils
2 | RED/BLU | AP3 | B+ from Engine Controls Relay to ECM | 2 | RED/BLU | AP4 | B+ from Engine Controls Relay to ECM
3-8 | -- | -- | Not Used | 3-8 | -- | -- | Not Used
9 | -- | -- | Not Used | 9 | BRN/WHT | XM799 | Serial Data
10 | BRN | X756 | Ignition Voltage from Fuse #3 | 10 | BRN | X756 | Ignition Voltage from Fuse #3
11-14 | -- | -- | Not Used | 11-14 | -- | -- | Not Used
15 | BLU | P901 | Instrument Cluster to Coolant Temperature Sensor | 15 | BLU | P900 | Instrument Cluster to Coolant Temperature Sensor
16 | -- | -- | Not Used | 16 | -- | -- | Not Used
17 | BRN/YEL | XP952 | Heated Oxygen Signal | 17 | BRN/BLU | XP34 | Heated Oxygen Sensor Signal
18-20 | -- | -- | Not Used | 18-20 | -- | -- | Not Used

#### Inline Connector C106

Connector Part Information |

• | ZFW 20-2

• | 20 WAY F (BLU)

Connector Part Information

• | ZMW 20-2

• | 20 WAY M (BLU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BLK/RED | FA500 | Positive Ignition Voltage | 1 | BLK/RED | FA700 | Positive Ignition Voltage
2 | BLK/RED | FA501 | Transmission Position Signal | 2 | BLK/RED | FA501 | Transmission Position Signal
3 | BLU/YEL | PB743 | 2-3 Shift Solenoid Control | 3 | BLU/YEL | PB743 | 2-3 Shift Solenoid Control
4 | GRY/BLK | RF745 | Band Apply Solenoid Control | 4 | GRY/BLK | RF745 | Band Apply Solenoid Control
5 | BLU/BLK | PF754 | 12 Volt Reference from TCM | 5 | BLU/BLK | PF754 | 12 Volt Reference from TCM
6 | BLU/WHT | PM748 | 1-2 and 3-4 Shift Solenoid Control | 6 | BLU/WHT | PM748 | 1-2 and 3-4 Shift Solenoid Control
7 | BLK/YEL | FB738 | TCC Solenoid Control | 7 | BLK/YEL | FB738 | TCC Solenoid Control
8 | BLK/PPL | FY740 | Pressure Control Solenoid Signal HIGH | 8 | BLK/PPL | FY740 | Pressure Control Solenoid Signal HIGH
9 | BLK/BLU | FP722 | Transmission Fluid Temperature Signal | 9 | BLK/BLU | FP722 | Transmission Fluid Temperature Signal
10 | GRY/RED | RA741 | Pressure Control Solenoid Signal LOW | 10 | GRY/RED | RA741 | Pressure Control Solenoid Signal LOW
11 | BLU/GRN | PU705 | Output Shaft Speed Signal | 11 | BLU/GRN | PU714 | Output Shaft Speed Signal
12 | BLK | S10 | Shield Wire | 12 | BLK | S40 | Shield Wire
13 | WHT/BLK | MF757 | B+ Ignition to Automatic Transmission Switch | 13 | WHT/BLK | MF757 | B+ Ignition to Automatic Transmission Switch
14 | BLK/YEL | FB708 | Transmission Position Signal | 14 | BLK/YEL | FB708 | Transmission Position Signal
15 | BLK/YEL | FB703 | Output Shaft Speed Signal | 15 | BLK/YEL | FB720 | Output Shaft Speed Signal
16 | -- | -- | Not Used | 16 | -- | -- | Not Used
17 | GRY | R733 | Transmission Position Signal | 17 | GRY | R733 | Gear Position Input Signal
18 | BLK/BLU | FP733 | Transmission Position Signal | 18 | BLK/BLU | FP10 | Gear Position Input Signal
19 | BLK/GRN | FU726 | Transmission Position Signal | 19 | BLK/GRN | FU2 | Gear Position Input Signal
20 | BRN/GRN | XU716 | Transmission Fluid Temperature Signal | 20 | BRN/GRN | XU716 | Transmission Fluid Temperature Signal

#### Inline Connector C108

Connector Part Information |

• | ZPF 2-3

• | 2 WAY F (BLK)

Connector Part Information

• | ZPM 2-3

• | 2 WAY M (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | X1 | Heated Nozzle On Signal | A | BRN | X600 | Heated Nozzle On Signal
B | BLK | F1 | Ground to G103 | B | BLK | F600 | Ground to G103

#### Inline Connector C110

Connector Part Information |

• | ZP 9-22

• | 9 WAY F (BLK)

Connector Part Information

• | ZM 9-22

• | 9 WAY M (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BRN/GRY | XR620 | Secondary Air Injection Pump Control | 1 | BRN/GRY | XR200 | Secondary Air Injection Pump Control
2 | BLK/BLU | FP120 | A/C Load Signal | 2 | BLK/BLU | FP99 | A/C Load Signal
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | BLK/WHT | FM98 | A/C Request Signal | 4 | BLK/WHT | FM99 | A/C Request Signal
5 | BRN/PPL | XY360 | A/C Compressor Relay Control Signal | 5 | BRN/PPL | XY107 | A/C Compressor Relay Control Signal
6 | RED/BLU | AP888 | B+ from Engine Controls Relay K43 | 6 | RED/BLU | AP200 | B+ from Engine Controls Relay K43
7-9 | -- | -- | Not Used | 7-9 | -- | -- | Not Used

#### Inline Connector C111

Connector Part Information |

• | ZFW 6-3

• | 6 WAY F (GRY)

Connector Part Information

• | ZMW 6-3

• | 6 WAY M (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BRN | X68 | B+ from Fuse #10 | 1 | BRN | X67 | B+ from Fuse #10
2 | BLK/YEL | FB1 | Interval Switch Signal | 2 | BLK/YEL | FB3 | Interval Switch Signal
3 | BLU | P2 | Windshield Wiper/Washer Mist Signal | 3 | BLU | P2 | Windshield Wiper/Washer Mist Signal
4 | GRN | U10 | Windshield Washer Motor Signal | 4 | GRN | U6 | Windshield Washer Motor Signal
5 | BLK/RED | FA1 | Windshield Washer Pump Signal | 5 | BLK/RED | FA5 | Windshield Washer Pump Signal
6 | BLK/PPL | FY1 | B+ from Fuse #9 | 6 | BLK/PPL | FY3 | B+ from Fuse #9

#### Inline Connector C112

Connector Part Information |

• | 12059472

• | ASM 7F M/P MIXED (BLK)

Connector Part Information

• | 12052200

• | ASM 7M M/P MIXED (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN/YEL | XB17 | Fuel Injector #1 Control | A | BRN/YEL | XB17 | Fuel Injector #1 Control
B | BRN/GRN | XU16 | Fuel Injector #2 Control | B | BRN/GRN | XU16 | Fuel Injector #2 Control
C | BRN/BLU | XP35 | Fuel injector #3 control | C | BRN/BLU | XP35 | Fuel injector #3 control
D | BRN/RED | XA34 | Fuel Injector #4 Control | D | BRN/RED | XA34 | Fuel Injector #4 Control
E | BRN/BLK | XF15 | Fuel Injector #5 Control | E | BRN/BLK | XF15 | Fuel Injector #5 Control
F | BRN/PPL | XY33 | Fuel Injector #6 Control | F | BRN/PPL | XY33 | Fuel Injector #6 Control
G | RED/BLU | AP751 | B+ from Relay K43 | G | RED/BLU | AP751 | B+ from Relay K43

#### Inline Connector C200A

Connector Part Information |

• | ZF 80-1

• | 62 WAY F (BLK)

Connector Part Information

• | ZM 80-1

• | 62 WAY M (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BLU | P1 P5 (W8Y) | LH Front Door Speaker Feed | 1 | BLU | P1 | LH Front Door Speaker Feed
2 | BRN/BLU | XP4 XP5 (W8Y) | LH Front Door Speaker Return | 2 | BRN/BLU | XP1 | LH Front Door Speaker Return
3 | WHT | M64 | B+ When High Beams are ON | 3 | WHT | M3 | B+ When High Beams are ON
4 | BLK/RED | FA3 | WSWA Pump Signal | 4 | BLK/RED | FA80 | WSWA Pump Signal
5 | BRN/WHT | XM700 XM15 | Serial Data | 5 | BRN/WHT | XM700 | Serial Data
6 | WHT | M42 M43 (W8Y) | RH Rear Door Speaker Feed | 6 | WHT | M42 | RH Rear Door Speaker Feed
7 | BRN/WHT | XM42 XM43 (W8Y) | RH Rear Door Speaker Return | 7 | BRN/WHT | XM42 | RH Rear Door Speaker Return
8 | RED | A701 | B+ fro Fuse #25 | 8 | RED | A700 | B+ fro Fuse #25
9 | BRN/WHT | XM30 | Horn Relay Control Signal | 9 | BRN/WHT | XM70 | Horn Relay Control Signal
10 | BLU | P11 | Solar/Twilight Sensor Ground | 10 | BLU | P11 | Solar/Twilight Sensor Ground
11 | GRY/RED | RA30 | B+ When Parklamps are ON | 11 | GRY/RED | RA2 | B+ When Parklamps are ON
12 | BRN | X79 X701 | B+ from Fuse #13 | 12 | BRN | X999 | B+ from Fuse #13
13 | YEL | B8 B9 (W8Y) | RH Front Door Speaker Feed | 13 | YEL | B10 | RH Front Door Speaker Feed
14 | BRN/YEL | XB10 XB12 (W8Y) | RH Front Door Speaker Return | 14 | BRN/YEL | XB10 | RH Front Door Speaker Return
15 | BRN/WHT | XM300 | Serial Data | 15 | BRN/WHT | XM218 | Serial Data
16 | BLU/BLK | PF900 | 5V Reference | 16 | BLU/BLK | PF901 | 5V Reference
17 | BRN/PPL | XY802 | Low When High Beams are ON | 17 | BRN/PPL | XY802 | Low When High Beams are ON
18 | BRN | X838 | B+ from Fuse #10 | 18 | BRN | X826 | B+ from Fuse #10
19 | YEL | B60 | Low Beams ON/OFF Signal | 19 | YEL | B899 | Low Beams ON/OFF Signal
20 | WHT | M69 | High Beams ON Signal | 20 | WHT | M60 | High Beams ON Signal
21 | BRN/BLU | XP900 | Rear Compartment Courtesy Switch Signal | 21 | BRN/BLU | XP901 | Rear Compartment Courtesy Switch Signal
22 | RED/YEL | AB810 | TWS ON/OFF Signal | 22 | RED/YEL | AB810 | TWS ON/OFF Signal
23 | YEL | B900 | Gear Out of Park Signal | 23 | YEL | B900 | Gear Out of Park Signal
25 | BLK/BRN | FX810 | TWS Delay SIgnal | 25 | BLK/BRN | FX810 | TWS Delay SIgnal
26 | BRN/RED | XA105 | Traction Control ON Signal | 26 | BRN/RED | XA105 | Traction Control ON Signal
27 | BLK/GRN | FU90 | Driver Seat Heater Switch Output | 27 | BLK/GRN | FU900 | Driver Seat Heater Switch Output
28 | BRN/BLU | XP840 | Security Lamp Indicator | 28 | BRN/BLU | XP840 | Security Lamp Indicator
29 | BRN/BLK | XF830 | TWS Indicator | 29 | BRN/BLK | XF830 | TWS Indicator
30 | RED/BLU | AP807 | Rear Compartment Open Signal | 30 | RED/BLU | AP822 | Rear Compartment Open Signal
31 | BRN/PPL | XY800 | Delay Interior Relay Signal | 31 | BRN/PPL | XY800 | Delay Interior Relay Signal
32 | RED | A12 | B+ from Fuse #24 | 32 | RED | A999 | B+ from Fuse #24
33 | BLK/BRN | FX750 | Stoplamp Switch Signal | 33 | BLK/BRN | FX899 | Stoplamp Switch Signal
34 | BRN/BLU | XP33 | TWS Day/NIght Signal | 34 | BRN/BLU | XP830 | TWS Day/NIght Signal
35 | BLK/RED | FA90 | Driver Seat Heater Switch Input | 35 | BLK/RED | FA90 | Driver Seat Heater Switch Input
36 | BRN/WHT | XM600 | Serial Data | 36 | BRN/WHT | XM830 | Serial Data
37 | BRN/WHT | XM899 | Horn Control Relay Signal | 37 | BRN/WHT | XM899 | Horn Control Relay Signal
39 | RED/BLU | AP100 | B+ from Engine Controls Power Relay | 39 | RED/BLU | AP888 | B+ from Engine Controls Power Relay
40 | BRN/PPL | XY801 | Interior Lamps Relay Signal | 40 | BRN/PPL | XY801 | Interior Lamps Relay Signal
41 | BLK/PPL | FY810 | TWS Return | 41 | BLK/PPL | FY810 | TWS Return
42 | RED/WHT | AM813 | Low When Parklamps are ON | 42 | RED/WHT | AM899 | Low When Parklamps are ON
43 | BRN/PPL | XY112 | Interior Lamps ON/OFF Signal | 43 | BRN/PPL | XY112 | Interior Lamps ON/OFF Signal
44 | BRN/BLU | XP803 | Low When Interior Lamps are ON | 44 | BRN/BLU | XP803 | Low When Interior Lamps are ON
45 | RED/YEL | AB11 | SIR Front Side Impact Module (LH) Output | 45 | RED/YEL | AB11 | SIR Front Side Impact Module (LH) Output
46 | RED/YEL | XB100 | SIR Front Side Impact Module (LH) Input | 46 | RED/YEL | XB100 | SIR Front Side Impact Module (LH) Input
47 | RED/WHT | AM13 | SIR Front Side Impact Module (RH) Input | 47 | RED/WHT | AM13 | SIR Front Side Impact Module (RH) Input
48 | BRN/WHT | XM14 | SIR Front Side Impact Module (RH) Output | 48 | BRN/WHT | XM14 | SIR Front Side Impact Module (RH) Output
49 | BRN/YEL | XB105 | ABS Indicator Signal | 49 | BRN/YEL | XB105 | ABS Indicator Signal
50 | BRN/YEL | XB950 | Passenger Seat Belt Pretensioner Output | 50 | BRN/YEL | XB901 | Passenger Seat Belt Pretensioner Output
51 | RED/YEL | AB950 | Passenger Seat Belt Pretensioner Input | 51 | RED/YEL | AB900 | Passenger Seat Belt Pretensioner Input
52 | RED/WHT | AM950 | Driver Seat Pretensioner Input | 52 | RED/WHT | AM900 | Driver Seat Pretensioner Input
53 | BRN/PPL | XY29 | ABS Can Interface High | 53 | BRN/PPL | XY888 | ABS Can Interface High
54 | BRN/GRY | XR12 | ABS Can Interface Low | 54 | BRN/GRY | XR888 | ABS Can Interface Low
55 | BRN/WHT | XM950 | Driver Seat Belt Pretensioner Output | 55 | BRN/WHT | XM901 | Driver Seat Belt Pretensioner Output
56 | YEL | B41 | SIR Side Impact Sensor (LH) Input | 56 | YEL | B41 | SIR Side Impact Sensor (LH) Input
57 | BRN/YEL | XB4 | ABS Indicator SIgnal | 57 | BRN/YEL | XB305 | ABS Indicator SIgnal
58 | BRN/YEL | XB42 | SIR Side Impact Sensor (LH) Output | 58 | BRN/YEL | XB42 | SIR Side Impact Sensor (LH) Output
59 | BLK/BLU | FP7 | Passenger Seat Heater Switch Output | 59 | BLK/BLU | FP7 | Passenger Seat Heater Switch Output
60 | BRN/WHT | XM430 | SIR Side Impact Sensor (RH) Input | 60 | BRN/WHT | XM430 | SIR Side Impact Sensor (RH) Input
61 | WHT | M44 | SIR Side Impact Sensor (RH) Output | 61 | WHT | M44 | SIR Side Impact Sensor (RH) Output
62 | GRY/WHT | RM1 | Interior Lamps ON/OFF Signal | 62 | GRY/WHT | RM1 | Interior Lamps ON/OFF Signal
63 | BLU/RED | PA60 | Rear Sunshade Switch Signal | 63 | BLU/RED | PA6 | Rear Sunshade Switch Signal
64 | BRN/PPL | XY999 | Serial Data | 64 | BRN/PPL | XY999 | Serial Data
65 | BRN/YEL | XB3 | Windshield Washer Minimum Capacity Signal | 65 | BRN/YEL | XB3 | Windshield Washer Minimum Capacity Signal
66 | YEL/RED | BA2 | Brake Wear Sensor Signal | 66 | YEL/RED | BA2 | Brake Wear Sensor Signal
67 | BLU/WHT | PM4 | Outside Temperature Signal | 67 | BLU/WHT | PM4 | Outside Temperature Signal
68 | BLK/YEL | FB70 | Passenger Seat Heater Switch Input | 68 | BLK/YEL | FB70 | Passenger Seat Heater Switch Input
69 | GRY/BLK | RF999 | B+ to LH Cornering Lamps | 69 | GRY/BLK | RF998 | B+ to LH Cornering Lamps
70 | GRY/RED | RA999 | B+ to RH Cornering Lamps | 70 | GRY/RED | RA998 | B+ to RH Cornering Lamps
71 | RED/BLU | AP4 | B+ to Fuse #18 | 71 | RED/BLU | AP11 | B+ to Fuse #18
72 | RED | A816 | B+ to Fuse #28 | 72 | RED | A13 | B+ to Fuse #28
73 | BRN | X15 | B+ When Defogger is ON | 73 | BRN | X16 | B+ When Defogger is ON
74 | RED | A48 | B+ to Fuse #1 | 74 | RED | A10 | B+ to Fuse #1
75 | RED | A49 | B+ to Fuse #7 | 75 | RED | A2 | B+ to Fuse #7
76 | RED | A65 | B+ to Fuse #35 | 76 | RED | A65 | B+ to Fuse #35
77 | BRN | X300 | B+ to Fuse #15 | 77 | BRN | X100 | B+ to Fuse #15
78 | RED | A240 | B+ to Fuse #20 | 78 | RED | A240 | B+ to Fuse #20
79 | BLK/BLU | FP2 | Fog Lamp Output | 79 | BLK/BLU | FP1 | Fog Lamp Output
80 | BLK/WHT | FM19 | LH High Beam Headlamp Signal | 80 | BLK/WHT | FM13 | LH High Beam Headlamp Signal

#### Inline Connector C200B

Connector Part Information |

• | ZF 43-2

• | 43 WAY F (BLK)

Connector Part Information

• | ZM 43-2

• | 43 WAY M (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BRN/GRN | XU42 XU43 (W8Y) | LH Rear Door Speaker Return | 1 | BRN/GRN | XU42 | LH Rear Door Speaker Return
2 | GRN | U41 U42 (W8Y) | LH Rear Door Speaker Feed | 2 | GRN | U42 | LH Rear Door Speaker Feed
3 | BLK/WHT | FM100 | B+ from Fuse #11 | 3 | BLK/WHT | FM10 | B+ from Fuse #11
4 | WHT | M808 | Fast Wiper Signal | 4 | WHT | M808 | Fast Wiper Signal
5 | Not Used
6 | RED | A24 | B+ from Fuse #4 | 6 | RED | A100 | B+ from Fuse #4
7 | RED | A892 | Low When High Beams are ON | 7 | RED | A888 | Low When High Beams are ON
8 | BRN | X43 | ALC Compressor Motor Signal | 8 | BRN | X101 | ALC Compressor Motor Signal
9 | RED | A301 | B+ from Fuse #17 | 9 | RED | A30 | B+ from Fuse #17
10 | WHT/BLK | MF757 | B+ With Automatic Transmission Range Switch in Reverse | 10 | WHT/BLK | MF900 MF10 (W8Y) | B+ With Automatic Transmission Range Switch in Reverse
11 | RED | A101 | B+ from Fuse #27 | 11 | RED | A295 | B+ from Fuse #27
12 | BRN/WHT | XM999 | Serial Data | 12 | BRN/WHT | XM55 | Serial Data
13 | BLU/RED | PA10 | Vehicle Speed Signal | 13 | BLU/RED | PA901 PA909 | Vehicle Speed Signal
14 | YEL | B810 | Wiper 1 Interval Signal | 14 | YEL | B810 | Wiper 1 Interval Signal
15 | YEL | B11 | B+ When Low Beams are ON | 15 | YEL | B1 B11 (T97) | B+ When Low Beams are ON
16 | BRN/YEL | XB910 | Headlamps ON Required Signal | 16 | BRN/YEL | XB910 | Headlamps ON Required Signal
17 | BLK/RED | FA202 | B+ from Fuse #19 | 17 | BLK/RED | FA202 | B+ from Fuse #19
18 | YEL | B22 | B+ When Low Beams are ON | 18 | YEL | B3 B30 (T97) | B+ When Low Beams are ON
19 | WHT | M8 | B+ When High Beams are ON | 19 | WHT | M2 | B+ When High Beams are ON
20 | BLK/YEL | FB10 | B+ to Auxiliary Brake Lamp | 20 | BLK/YEL | FB303 | B+ to Auxiliary Brake Lamp
21 | GRY/YEL | RF30 | B+ When Parklamps are ON | 21 | GRY/YEL | RF2 | B+ When Parklamps are ON
22 | BLU/BLK | PF1 | Fuel Gauge Level Signal | 22 | BLU/BLK | PF12 | Fuel Gauge Level Signal
23 | BLK/GRN | FU11 | RH Turn and Taillamp Signal | 23 | BLK/GRN | FU1 | RH Turn and Taillamp Signal
24 | BLK/WHT | FM12 | LH Turn and Taillamp Signal | 24 | BLK/WHT | FM1 | LH Turn and Taillamp Signal
25 | BLK/RED | FA825 | Brake to Shift Indicator | 25 | BLK/RED | FA399 | Brake to Shift Indicator
26 | BRN/GRN | XU900 | Sensor Ground | 26 | BRN/GRN | XU901 | Sensor Ground
27 | GRY/GRN | RU10 | B+ When Parklamps are ON | 27 | GRY/GRN | RU7 | B+ When Parklamps are ON
28 | BRN/YEL | XB900 | Fuel Pressure Sensor Signal | 28 | BRN/YEL | XB902 | Fuel Pressure Sensor Signal
29 | BRN/BLK | XF18 | Control Circuit for Evaporative Tank (EVAP) Solenoid Valve | 29 | BRN/BLK | XF888 | Control Circuit for Evaporative Tank (EVAP) Solenoid Valve
30 | WHT | M3 | High Beams ON/OFF Signal | 30 | WHT | M50 | High Beams ON/OFF Signal
31 | BLK/RED | FA812 | Rear Compartment Lid Release Signal | 31 | BLK/RED | FA812 | Rear Compartment Lid Release Signal
32 | RED/WHT | AM110 | Radio ON Signal | 32 | RED/WHT | AM42 | Radio ON Signal
33 | GRY/YEL | RB200 | Dimmer Signal | 33 | GRY/YEL | RB200 | Dimmer Signal
34 | YEL | B56 | ALC Relay Control Signal | 34 | YEL | B25 | ALC Relay Control Signal
35 | BRN/RED | XA810 | Low Beams Relay Signal | 35 | BRN/RED | XA810 | Low Beams Relay Signal
36 | BRN/WHT | XM810 | Low When Parklamps are ON | 36 | BRN/WHT | XM810 | Low When Parklamps are ON
37 | BRN/BLU | XP810 | Battery Guard Signal | 37 | BRN/BLU | XP811 | Battery Guard Signal
38 | BRN/WHT | XM111 | Serial Data | 38 | BRN/WHT | XM900 | Serial Data
39 | BRN/PPL | XY2 | Leveling Indicator Signal | 39 | BRN/PPL | XY1 | Leveling Indicator Signal
40 | RED/WHT | AM810 | Low When Parklamps are ON | 40 | RED/WHT | AM810 | Low When Parklamps are ON
41 | BLK/RED | FA811 | Fuel Door Release Signal | 41 | BLK/RED | FA811 | Fuel Door Release Signal
42 | BRN/WHT | XM200 | LH Turn Signal Lamp Signal | 42 | BRN/WHT | XM200 | LH Turn Signal Lamp Signal
43 | BRN/BLK | XF20 | Seat Belt Warning Signal | 43 | BRN/BLK | XF21 | Seat Belt Warning Signal

#### Inline Connector C201

Connector Part Information |

• | ZPF 2-50

• | 2 WAY F (BLK)

Connector Part Information

• | ZPF 2-50

• | 2 WAY M (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | S43 | Shield Ground | A | BLK | SO2 | Shield Ground
B | BRN/GRY | XR109 | Microphone Signal | B | BRN/GRY | XR2 | Microphone Signal

#### Inline Connector C205

Connector Part Information |

• | ZF 9 -23

• | 9 WAY F (WHT)

Connector Part Information

• | ZM 9 -23

• | 9 WAY M (WHT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | GRN | U900 | Lifting Magnet Control Signal | 1 | GRN | -- | Lifting Magnet Control Signal
2 | BLU | P100 | Sport Mode Switch Input | 2 | BLU | -- | Sport Mode Switch Input
3-5 | -- | -- | Not Used | 3-5 | -- | -- | Not Used
6 | BLK | F950 | Ground to G103 | 6 | BRN | -- | Ground to G103
7 | YEL | B901 | Ground Supply for Fuel Tank Filler Release Switch | 7 | WHT | -- | Ground Supply for Fuel Tank Filler Release Switch
8 | BLK/BRN | FX900 | B+ When Stoplamp Switch is Closed | 8 | BLK/YEL | -- | B+ When Stoplamp Switch is Closed
9 | YEL | B900 | Gear Out of Park Signal to BCM | 9 | BLU | -- | Gear Out of Park Signal to BCM

#### Inline Connector C207 (With Side Airbags)

Connector Part Information |

• | ZF 9 -34

• | 9 WAY F (BLU)

Connector Part Information

• | ZM9 -34

• | 9 WAY M (BLU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BRN/YEL | XB950 | Passenger Seat Pretensioner Signal LOW | 1 | BRN/YEL | XB901 | Passenger Seat Pretensioner Signal LOW
2 | RED/YEL | AB950 | Passenger Seat Pretensioner Signal HIGH | 2 | RED/YEL | AB900 | Passenger Seat Pretensioner Signal HIGH
3 | RED/WHT | AM950 | Driver Seat Pretensioner Signal HIGH | 3 | RED/WHT | AM900 | Driver Seat Pretensioner Signal HIGH
4 | BRN/WHT | XM950 | Driver Seat Pretensioner Signal LOW | 4 | BRN/WHT | XM901 | Driver Seat Pretensioner Signal LOW
5 | YEL | B41 | Driver Seat Side Impact Sensor Signal | 5 | YEL | B41 | Driver Seat Side Impact Sensor Signal
6 | BRN/YEL | XB42 | Driver Seat Side Impact Sensor Signal | 6 | BRN/YEL | XB42 | Driver Seat Side Impact Sensor Signal
7 | BRN/WHT | XM430 | Passenger Seat Side Impact Sensor Signal | 7 | BRN/WHT | XM430 | Passenger Seat Side Impact Sensor Signal
8 | WHT | M44 | Passenger Seat Side Impact Sensor Signal | 8 | WHT | M44 | Passenger Seat Side Impact Sensor Signal
9 | BRN/PPL | XY999 | ONSTAR Signal | 9 | BRN/PPL | XY999 | ONSTAR Signal

#### Inline Connector C208 (With Side Airbags)

Connector Part Information |

• | ZF 2-15

• | 2 WAY F (YEL)

Connector Part Information

• | ZM 2-15

• | 2 WAY M (YEL)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RED/YEL | AB11 | Driver Side HIGH Signal | 1 | RED/YEL | AB11 | Driver Side HIGH Signal
2 | BRN/YEL | XB100 | Driver Side LOW Signal | 2 | BRN/YEL | XB100 | Driver Side LOW Signal

#### Inline Connector C209 (With Side Airbags)

Connector Part Information |

• | ZF 2-16

• | 2 WAY F (GRY)

Connector Part Information

• | ZM 2-16

• | 2 WAY M

• | GRY

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RED/WHT | AM13 | Passenger Side HIGH Signal | 1 | RED/WHT | AM13 | Passenger Side HIGH Signal
2 | BRN/WHT | XM14 | Passenger Side LOW Signal | 2 | BRN/WHT | XM14 | Passenger Side LOW Signal

#### Inline Connector C210

Connector Part Information |

• | ZF 42-3

• | 42 WAY F (BLK)

Connector Part Information

• | ZM 42-3

• | 42 WAY M (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RED | A202 | B+ from Fuse #6 | 1 | RED | A200 | B+ from Fuse #6
2 | BLK | F102 | Ground to G201 | 2 | BLK | F100 | Ground to G201
3 | BRN/WHT | XM160 | Serial Data | 3 | BRN/WHT | XM15 | Serial Data
4 | BRN/WHT | XM45 | Serial Data | 4 | BRN/WHT | XM45 | Serial Data
5 | BLK | S45 | Shield Wire | 5 | BLK | S45 | Shield Wire
6 | WHT | M90 | Chime Input (Not Used) | 6 | WHT | M90 | Chime Input (Not Used)
7 | BRN/WHT | XM93 | Chime Input (Not Used) | 7 | BRN/WHT | XM90 | Chime Input (Not Used)
8 | BLK | S46 | Shield Wire | 8 | BLK | S46 | Shield Wire
9 | WHT | M91 | Sound Processor Signal RH (-) | 9 | WHT | M91 | Sound Processor Signal RH (-)
10 | BRN/WHT | XM91 | Sound Processor Signal RH (+) | 10 | BRN/WHT | XM91 | Sound Processor Signal RH (+)
11 | BLK | S47 | Shield Wire | 11 | BLK | S47 | Shield Wire
12 | WHT | M92 | Sound Processor Signal LH (-) | 12 | WHT | M92 | Sound Processor Signal LH (-)
13 | BRN/WHT | XM92 | Sound Processor Signal LH (+) | 13 | BRN/WHT | XM92 | Sound Processor Signal LH (+)
14 | BRN/WHT | XM43 | RH Rear Door Speaker Signal (-) | 14 | BRN/WHT | XM43 | RH Rear Door Speaker Signal (-)
15 | WHT | M43 | RH Rear Door Speaker Signal (+) | 15 | WHT | M43 | RH Rear Door Speaker Signal (+)
16 | BRN/BLU | XP5 | LH Front Door Speaker Signal (-) | 16 | BRN/BLU | XP2 | LH Front Door Speaker Signal (-)
17 | BLU | P5 | LH Front Door Speaker Signal (+) | 17 | BLU | P2 | LH Front Door Speaker Signal (+)
18 | BRN/YEL | XB12 | RH Front Door Speaker Signal (-) | 18 | BRN/YEL | XB11 | RH Front Door Speaker Signal (-)
19 | RED | A201 | B+ from Fuse #8 | 19 | RED | A201 | B+ from Fuse #8
20 | BLK | F101 | Ground to G201 | 20 | BLK | F101 | Ground to G201
21 | -- | -- | Not Used | 21 | -- | -- | Not Used
22 | YEL | B9 | RH Front Door Speaker Signal (+) | 22 | YEL | B4 | RH Front Door Speaker Signal (+)
23 | BRN/GRN | XU43 | LH Rear Door Speaker Signal (-) | 23 | BRN/GRN | XU43 | LH Rear Door Speaker Signal (-)
24 | GRN | U42 | LH Rear Door Speaker Signal (+) | 24 | GRN | U43 | LH Rear Door Speaker Signal (+)
25 | -- | -- | Not Used | 25 | -- | -- | Not Used
26 | YEL | B20 | CD Player Signal | 26 | YEL | B20 | CD Player Signal
27-28 | -- | -- | Not Used | 27-28 | -- | -- | Not Used
29 | BRN | X405 | B+ from Fuse #14 | 29 | BRN | X10 | B+ from Fuse #14
30 | BLK | F405 | Ground to G201 | 30 | BLK | F10 | Ground to G201
31 | RED | A406 | B+ from Multifunction Relay | 31 | RED | A406 | B+ from Multifunction Relay
32-42 | -- | -- | Not Used | 32-42 | -- | -- | Not Used

#### Inline Connector C301

Connector Part Information |

• | F 9-3

• | 9 WAY F (WHT)

Connector Part Information

• | M 9-3

• | 9 WAY M (WHT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | GRY | R2 | RH Rear Side Door Jamb Switch Signal | 1 | GRY | R18 | RH Rear Side Door Jamb Switch Signal
2 | RED/BLU | AP1 | RH Roof Rail Courtesy Lamp Signal | 2 | RED/BLU | AP809 | RH Roof Rail Courtesy Lamp Signal
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | BRN/BLU | XP1 | Rear Compartment Lid Open Signal | 4 | BRN/BLU | XP805 | Rear Compartment Lid Open Signal
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | BLK | F1 | Ground to G103 | 6 | BLK | F88 | Ground to G103
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | GRY | R1 | RH Rear Side Door Jamb Switch Signal | 8 | GRY | R16 | RH Rear Side Door Jamb Switch Signal
9 | -- | -- | Not Used | 9 | -- | -- | Not Used

#### Inline Connector C302

Connector Part Information |

• | F 9-3

• | 9 WAY F (WHT)

Connector Part Information

• | M 9-3

• | 9 WAY M (WHT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | GRY | R2 | LH Rear Side Door Jamb Switch Signal | 1 | GRY | R17 | LH Rear Side Door Jamb Switch Signal
2 | RED/BLU | AP1 | LH Roof Rail Courtesy Lamp Signal | 2 | RED/BLU | AP810 | LH Roof Rail Courtesy Lamp Signal
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | BRN/BLU | XP1 | Rear Compartment Lid Open Signal | 4 | BRN/BLU | XP804 | Rear Compartment Lid Open Signal
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | BLK | F1 | Ground to G103 | 6 | BLK | F84 | Ground to G103
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | GRY | R1 | LH Rear Side Door Jamb Switch Signal | 8 | GRY | R15 | LH Rear Side Door Jamb Switch Signal
9 | -- | -- | Not Used | 9 | -- | -- | Not Used

#### Inline Connector C303

Connector Part Information |

• | ZF 15-4

• | 15 WAY F (BLK)

Connector Part Information

• | ZM 15-4

• | 15 WAY M (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | YEL | B7 | Memory Programming Signal | 1 | YEL | B1 | Memory Programming Signal
2 | BLK/RED | FA804 | Doors Unlock Signal | 2 | BLK/RED | FA804 | Doors Unlock Signal
3 | BLK/YEL | FB805 | Doors Lock Signal | 3 | BLK/YEL | FB805 | Doors Lock Signal
4 | BLK | F19 | Ground | 4 | BLK | F3 | Ground
5 | GRY/GRN | RU15 | Window Up Signal | 5 | GRY/GRN | RU1, RU2 | Window Up Signal
6-7 | -- | -- | Not Used | 6-7 | -- | -- | Not Used
8 | RED | A21 | B+ from Fuse #7 | 8 | RED | A1 | B+ from Fuse #7
9 | BLU/RED | PA3 | Window Down Signal | 9 | BLU/RED | PA1, PA2 | Window Down Signal
10 | WHT | M3 | Rear Window Switch Enable Signal | 10 | WHT | M1 | Rear Window Switch Enable Signal
11 | GRY | R17 | Ground | 11 | GRY | R1 | Ground
12 | GRN | U42 | Speaker and Tweeter Feed Signal LH (+) | 12 | GRN | U2, | Speaker and Tweeter Feed Signal LH (+)
13 | BRN/GRN | XU42 | Speaker and Tweeter Return Signal LH (-) | 13 | BRN/GRN | XU2, | Speaker and Tweeter Return Signal LH (-)
14 | -- | -- | Not Used | 14 | -- | -- | Not Used
15 | RED/BLU | AP805 | B+ to Rear Door Lamp | 15 | RED/BLU | AP805 | B+ to Rear Door Lamp

#### Inline Connector C304

Connector Part Information |

• | ZF 15-4

• | 15 WAY F (BLK)

Connector Part Information

• | ZM 15-4

• | 15 WAY M (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | YEL | B8 | Memory Programming Signal | 1 | YEL | B1 | Memory Programming Signal
2 | BLK/RED | FA803 | Doors Unlock Signal | 2 | BLK/RED | FA804 | Doors Unlock Signal
3 | BLK/YEL | FB804 | Doors Lock Signal | 3 | BLK/YEL | FB805 | Doors Lock Signal
4 | BLK | F18 | Ground | 4 | BLK | F3 | Ground
5 | GRY/GRN | RU16 | Window Up Signal | 5 | GRY/GRN | RU1, RU2 | Window Up Signal
6-7 | -- | -- | Not Used | 6-7 | -- | -- | Not Used
8 | RED | A11 | B+ from Fuse #7 | 8 | RED | A1 | B+ from Fuse #7
9 | BLU/RED | PA4 | Window Down Signal | 9 | BLU/RED | PA1, PA2 | Window Down Signal
10 | WHT | M4 | Rear Window Switch Enable Signal | 10 | WHT | M1 | Rear Window Switch Enable Signal
11 | GRY | R18 | Ground | 11 | GRY | R1 | Ground
12 | GRN | M42 | Speaker and Tweeter Feed Signal RH (+) | 12 | GRN | U2 | Speaker and Tweeter Feed Signal RH (+)
13 | BRN/GRN | XM42 | Speaker and Tweeter Return Signal RH (-) | 13 | BRN/GRN | XU2 | Speaker and Tweeter Return Signal RH (-)
14 | -- | -- | Not Used | 14 | -- | -- | Not Used
15 | RED/BLU | AP804 | B+ to Rear Door Lamp | 15 | RED/BLU | AP805 | B+ to Rear Door Lamp

#### Inline Connector C305

Connector Part Information |

• | ZPF 2-50

• | 2 WAY F (BLK)

Connector Part Information

• | ZPM 2-50

• | 2 WAY M (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | F2 | Ground to G103 | A | BLK | F900 | Ground to G103
B | RED/BLU | AP2 | Sunshade ON Signal | B | RED/BLU | AP803 | Sunshade ON Signal

#### Inline Connector C310

Connector Part Information |

• | F 20-1

• | 20 WAY F (GRY)

Connector Part Information

• | M 20-1

• | 20 WAY M (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RED | A40 | B+ from Fuse #28 | 1 | RED | A40 | B+ from Fuse #28
2 | BRN | X13 | B+ from Fuse #15 | 2 | BRN | X13 | B+ from Fuse #15
3 | BLK | F40 | Ground to G103 | 3 | BLK | F40 | Ground to G103
4 | BRN/WHT | XM55 | Serial Data | 4 | BRN/WHT | XM55 | Serial Data
5 | GRY/WHT | RM12 | Door Open Signal | 5 | GRY/WHT | RM12 | Door Open Signal
6 | BLK/BRN | FX75 | Memory Potentiometer Signal | 6 | BLK/BRN | FX75 | Memory Potentiometer Signal
7 | BRN | X75 | Memory Potentiometer Signal | 7 | BRN | X75 | Memory Potentiometer Signal
8 | GRY/GRN | RU60 | RH Outside Rear View Mirror Memory Signal | 8 | GRY/GRN | RU60 | RH Outside Rear View Mirror Memory Signal
9 | GRY | R70 | RH Outside Rear View Mirror Memory Signal | 9 | GRY | R70 | RH Outside Rear View Mirror Memory Signal
10 | GRY/BLK | RF60 | Inside Rear View Mirror Memory Signal | 10 | GRY/BLK | RF60 | Inside Rear View Mirror Memory Signa
11 | GRY/YEL | RB60 | Inside rear view mirror memory signal | 11 | GRY/YEL | RB60 | Inside rear view mirror memory signal
12 | GRY/GRN | RU50 | Memory Potentiometer Signal | 12 | GRY/GRN | RU50 | Memory Potentiometer Signal
13 | GRY | R60 | Memory Potentiometer Signal | 13 | GRY | R60 | Memory Potentiometer Signal
14 | BLK/RED | FA75 | RH Outside Rear View Mirror Common | 14 | BLK/RED | FA75 | RH Outside Rear View Mirror Common
15 | GRN | U80 | LH Memory Mirror Control Signal | 15 | GRN | U80 | LH Memory Mirror Control Signal
16 | YEL | B12 | LH Memory Mirror Control Signal | 16 | YEL | B12 | LH Memory Mirror Control Signal
17 | BLU/WHT | PM60 | Inside Rear View Mirror Control Signal | 17 | BLU/WHT | PM60 | Inside Rear View Mirror Control Signal
18 | BLU/RED | PA60 | Inside Rear View Mirror Control Signal | 18 | BLU/RED | PA60 | Inside Rear View Mirror Control Signal
19 | BLU | P70 | RH Outside Rear View Mirror Control Signal | 19 | BLU | P70 | RH Outside Rear View Mirror Control Signal
20 | GRY | R65 | RH Outside Rear View Mirror Control Signal | 20 | GRY | R65 | RH Outside Rear View Mirror Control Signal

#### Inline Connector C320

Connector Part Information |

• | ZF 9-4

• | 9 WAY F (BLK)

Connector Part Information

• | ZM 9-4

• | 9 WAY M (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RED | A1 | B+ from Fuse #4 | 1 | RED | A6 | B+ from Fuse #4
2 | BLK/WHT | FM1 | LH Rear Seat Heater Switch Signal | 2 | BLK/WHT | FM300 | LH Rear Seat Heater Switch Signal
3 | BLK | F1 | Ground to G200 | 3 | BLK | F35 | Ground to G200
4 | BLK/YEL | FB2 | LH Rear Heater Relay ON Signal | 4 | BLK/YEL | FB32 | LH Rear Heater Relay ON Signal
5 | BRN | X1 | B+ from Fuse #15 | 5 | BRN | X33 | B+ from Fuse #15
6 | BLK/WHT | FM2 | RH Rear Seat Heater Switch Signal | 6 | BLK/WHT | FM31 | RH Rear Seat Heater Switch Signal
7 | BLK/RED | FA2 | RH Rear Heater Relay On Signal | 7 | BLK/RED | FA32 | RH Rear Heater Relay On Signal
8-9 | -- | -- | Not Used | 8-9 | -- | -- | Not Used

#### Inline Connector C400

Connector Part Information |

• | ZPF 8-1

• | 8 WAY F (BLK)

Connector Part Information

• | ZPM 8-1

• | 8 WAY M (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RED/BLU | AP11 | B+ from Fuse #18 | A | RED/BLU | AP10 | B+ from Fuse #18
B | BLK | F226 | Ground to G103 | B | BLK | F224 | Ground to G103
C | BLU/BLK | PF12 | Fuel Gauge Signal | C | BLU/BLK | PF11 | Fuel Gauge Signal
D | BRN/YEL | XB902 | Fuel Tank Pressure Signal | D | BRN/YEL | XB1 | Fuel Tank Pressure Signal
E | BRN/GRN | XU901 | Sensor Ground | E | BRN/GRN | XU1 | Sensor Ground
F | BLU/BLK | PF901 | 5V Reference | F | BLU/BLK | PF1 | 5V Reference
G | BLK | F225 | Ground to G400 | G | BLK | F30 | Ground to G400
H | -- | -- | Not Used | H | -- | -- | Not Used

#### Inline Connector C401

Connector Part Information |

• | ZFW 6-3

• | 6 WAY F (GRY)

Connector Part Information

• | ZMW 6-3

• | 6 WAY M (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | GRY/RED | RA1 | RH Rear Side Marker Lamp Signal | 1 | GRY/RED | RA20 | RH Rear Side Marker Lamp Signal
2 | GRY/GRN | RU1 | License Lamp Signal | 2 | GRY/GRN | RU11 | License Lamp Signal
3 | BLK/GRN | FU1 | RH Rear Side Marker Lamp Signal | 3 | BLK/GRN | FU30 | RH Rear Side Marker Lamp Signal
4 | GRY/BLK | RF1 | LH Rear Side Marker Lamp Signal | 4 | GRY/BLK | RF20 | LH Rear Side Marker Lamp Signal
5 | BLK | F1 | License Lamp Signal | 5 | BLK | F44 | License Lamp Signal
6 | BLK/WHT | FM1 | LH Rear Side Marker Lamp Signal | 6 | BLK/WHT | FM30 | LH Rear Side Marker Lamp Signal

#### Inline Connector C403

Connector Part Information |

• | ZPF 4-55

• | 4 WAY F (BLK)

Connector Part Information

• | ZPM 4-55

• | 4 WAY M (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BLK | F20 | Ground from G400 | 1 | BLK | F20 | Ground from G400
2 | BLU/RED | PA6 | Rear Sunshade Control Signal | 2 | BLU/RED | PA6 | Rear Sunshade Control Signal
3 | RED | A95 | Fused Battery Voltage | 3 | RED | A95 | Fused Battery Voltage
4 | -- | -- | Not Used | 4 | -- | -- | Not Used

#### Inline Connector C405

Connector Part Information |

• | Z 9-23

• | 9 WAY F (WHT)

Connector Part Information

• | Z 9-23

• | 9 WAY M (WHT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BLK/RED | FA807 | Rear Compartment Release Signal | 1 | BLK/RED | FA11 | Rear Compartment Release Signal
2 | BLK/YEL | FB15 | Auxiliary Brake Lamp Signal | 2 | BLK/YEL | FB5 | Auxiliary Brake Lamp Signal
3 | GRY/GRN | RU12 | Taillamp (Middle) Signal | 3 | GRY/BLK | RF1 | Taillamp (Middle) Signal
4 | BLK | F48 | Ground to G201 | 4 | BLK | F48 | Ground to G201
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | BLK/YEL | FB806 | Rear Compartment Release Signal | 6 | BLK/YEL | FB21 | Rear Compartment Release Signal
7 | BRN/BLU | XP901 | Rear Compartment Lamp Switch Signal | 7 | BRN/BLU | XP1 | Rear Compartment Lamp Switch Signal
8 | WHT/BLK | MF10 | Transmission Position Signal | 8 | WHT/BLK | MF10 | Transmission Position Signal
9 | BRN/WHT | XM9 | Rear Compartment Lamp Switch Signal | 9 | BRN/WHT | XM8 | Rear Compartment Lamp Switch Signal

#### Inline Connector C500

Connector Part Information |

• | ZFW 40-1

• | 40 WAY F (BLK)

Connector Part Information

• | ZMW 40-1

• | 40 WAY M (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BLK | F8 | Ground to G200 | 1 | BLK | F1 | Ground to G200
2 | RED | A1 | B+ from Fuse #1 | 2 | RED | A2 | B+ from Fuse #1
4 | GRY/YEL | RB43 | RH Front Side Door Window Switch Feed | 4 | GRY/YEL | RB43 | Front Side Door Window Switch Feed RH
5 | GRY | R11 | RH Outside Rear View Mirror Signal | 5 | GRY | R11 | RH Outside Rear View Mirror Signal
6 | GRY/WHT | RM20 | Driver Door Switch Input Signal | 6 | GRY/WHT | RM20 | Driver Door Switch Input Signal
7 | WHT | M5 | RH Rear Side Door Window Switch Input | 7 | WHT | M5 | Rear Side Door Window Switch Input RH
8 | GRY/GRN | RU15 | LH Rear Side Door UP Signal | 8 | GRY/GRN | RU15 | Rear Side Door UP Signal RH
9 | BLU/RED | PA3 | LH Rear Side Door Down Signal | 9 | BLU/RED | PA3 | LH Rear Side Door Down Signal
10 | GRY/GRN | RU16 | RH Rear Side Door UP Signal | 10 | GRY/GRN | RU16 | RH Rear Side Door UP Signal
11 | BLU/RED | PA4 | RH Rear Side Door Down Signal | 8-11 | BLU/RED | PA4 | RH Rear Side Door Down Signal
12 | BRN | X999 | B+ from Fuse #13 | 12 | BRN | X10 | B+ from Fuse #13
13 | BRN/PPL | XY810 | Key Disarm Signal | 13 | BRN/PPL | XY810 | Key Disarm Signal
14 | BRN/BLU | XP810 | Driver Door Courtesy Lmap Input | 14 | BRN/BLU | XP810 | Driver Door Courtesy Lmap Input
15 | BLK/BRN | FX805 | Serial Data | 15 | BLK/BRN | FX805 | Serial Data
16 | BLU/RED | PA1 | Window Down Signal | 16 | BLU/RED | PA1 | Window Down Signal
17 | GRY/GRN | RU6 | Window Up Signal | 17 | GRY/GRN | RU1 | Window Up Signal
18 | GRY | R20 | LH Front Side Door Jamb Switch Signal | 18 | GRY | R10 | LH Front Side Door Jamb Switch Signal
19 | BLK/WHT | FM10 | B+ from Fuse #11 | 19 | BLK/WHT | FM2 FM15 (W8Y) | B+ from Fuse #11
20 | BLU | P1 | Door Speaker and Tweeter Signal LH (+) | 20 | BLU | P1 | Door Speaker and Tweeter Signal LH (+)
21 | BLK/RED | FA7 | Outside Rear View Mirror Common | 21 | BLK/RED | FA7 | Outside Rear View Mirror Common
22 | BRN/BLU | XP1 | Door Speaker and Tweeter Signal LH (-) | 22 | BRN/BLU | XP1 | Door Speaker and Tweeter Signal LH (-)
23 | YEL | B6 | Door Open Signal | 23 | YEL | B12 | Door Open Signal
24 | YEL | B12 | Memory Control Signal | 24 | YEL | B81 (AG8) | Memory Control Signal
25 | BLK/YEL | FB803 | Window Actuator Signal | 25 | BLK/YEL | FB9 | Window Actuator Signal
26 | RED/BLU | AP806 | Door Lamp Signal | 26 | RED/BLU | AP888 | Door Lamp Signal
27 | BLU | P3 | Memory Control Signal | 27 | BLU | P3 | Memory Control Signal
29 | BLK/PPL | FY805 | Door Unlock Signal | 29 | BLK/PPL | FY805 | Door Unlock Signal
30 | GRY/YEL | RB80 | Driver Door Lock Switch Input | 30 |  | RB50 | Driver Door Lock Switch Input
32 | BLK/BRN | FX60 | Memory Potentiometer Signal | 32 | BLK/BRN | FX60 (AG8) | Memory Potentiometer Signal
33 | BRN | X60 | Memory Potentiometer Signal | 33 | BRN | X60(AG8) | Memory Potentiometer Signal
34 | BLK/RED | FA809 | Window Actuator Signal | 34 | BLK/RED | FA809 | Window Actuator Signal
35 | GRY/YEL | RB42 | LH Rear SIde Door Window Switch Lockout | 35 | GRY/YEL | RB42 | LH Rear SIde Door Window Switch Lockout
36 | GRY | R60 | Memory Potentiometer Signal | 36 | GRY | R60 (AG8) | Memory Potentiometer Signal
37 | GRN | U80 | Memory Control Signal | 37 | GRN | U100 (AG8) | Memory Control Signal
38 | GRY/GRN | RU50 | Memory Potentiometer Signal | 38 | GRY/GRN | RU60 (AG8) | Memory Potentiometer Signal
39 | BRN/YEL | XB42 | Side Impact Sensor Signal | 39 (AJ6) | BRN/YEL | XB42 | Side Impact Sensor Signal
40 | YEL | B41 | Side Impact Sensor Signal | 40 (AJ6) | YEL | B42 | Side Impact Sensor Signal

#### Inline Connector C600

Connector Part Information |

• | ZFW 40-1

• | 40 WAY F (BLK)

Connector Part Information

• | ZMW 40-2

• | 40 WAY M (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BLK | F9 | Ground to G200 | 1 | BLK | F1 | Ground to G200
2 | RED | A4 | B+ from Fuse #1 | 2 | RED | A2 | B+ from Fuse #1
4 | GRY/YEL | RB43 | LH Front SIde Door Window Switch Feed | 4 | GRY/YEL | RB43 | LH Front SIde Door Window Switch Feed
5 | GRY | R110 | RH Outside Rear View Mirror Signal | 5 | GRY | R4 R5 (AG8) | RH Outside Rear View Mirror Signal
14 | BRN/BLU | XP809 | Passenger Door Lamp Signal | 6 | BRN/BLU | XP810 | Passenger Door Lamp Signal
15 | BLK/BRN | FX804 | Door Lock Signal | 7 | BLK/BRN | FX805 | Door Lock Signal
16 | BLU/RED | PA1 | Window Down Signal | 16 | BLU/RED | PA20 | Window Down Signal
17 | GRY/GRN | RU6 | Window Up Signal | 17 | GRY/GRN | RU61 | Window Up Signal
19 | BLK/WHT | FM22 | B+ from Fuse #11 | 19 | BLK/WHT | FM2 FM20 (AG8) | B+ from Fuse #11
20 | YEL | B10 | Door Speaker and Tweeter Signal RH (+) | 20 | YEL | B1 | Door Speaker and Tweeter Signal RH (+)
21 | BLK/RED | FA700 | Outside Rear View Mirror Common | 21 | BLK/RED | FA4 FA65 (AG8) | Outside Rear View Mirror Common
22 | BRN/YEL | XB10 | Door Speaker and Tweeter Signal RH (-) | 22 | BRN/YEL | XB1 | Door Speaker and Tweeter Signal RH (-)
23 | YEL | B5 | Door Open Signal | 23 | YEL | B14 | Door Open Signal
25 | BLK/YEL | FB802 | Window Actuator Signal | 25 | BLK/YEL | FB9 | Window Actuator Signal
26 | RED/BLU | AP807 | Door Lamp Signal | 26 | RED/BLU | AP888 | Door Lamp Signal
27 | BLU | P30 | Memory Control Signal | 27 | BLU | P2 P10 (AG8) | Memory Control Signal
29 | BLK/PPL | FY804 | Door Unlock Signal | 29 | BLK/PPL | FY805 | Door Unlock Signal
32 | BLK/BRN | FX65 | Memory Potentiometer Signal | 32 | BLK/BRN | FX65(AG8) | Memory Potentiometer Signal
33 | BRN | X65 | Memory Potentiometer Signal | 33 | BRN | X65 (AG8) | Memory Potentiometer Signal
34 | BLK/RED | FA802 | Window Actuator Signal | 34 | BLK/RED | FA809 | Window Actuator Signal
36 | GRY | R70 | Memory Potentiometer Signal | 36 | GRY | R70 (AG8) | Memory Potentiometer Signal
38 | GRY/GRN | RU60 | Memory Potentiometer Signal | 38 | GRY/GRN | RU60 (AG8) | Memory Potentiometer Signal
39 | BRN/WHT | XM430 | Side Impact Sensor Signal | 39 | BRN/WHT | XM42(AJ6) | Side Impact Sensor Signal
40 | WHT | M44 | Side Impact Sensor Signal | 40 | WHT | M42 (AJ6) | Side Impact Sensor Signal