For 1990-2009 cars

### Circuit Description

When the automatic level control (ALC) sensor detects an out of trim condition, the auto level control relay K19 energizes to provide B+ to the auto level control air compressor. The automatic ALC sensor continuously monitors the controlling circuitry to determine if there is B+ present for a compress sequence or an air replenishment cycle (ARC).

### Conditions for Setting the DTC

The sensor detects that the relay output is not pulled down to ground when the sensor output is active.

### Action Taken When the DTC Sets

• | The LEVELING indicator lamp flashes.

• | The sensor's discrete low side output drive for the relay is disabled.

• | The sensor continuously attempts to recover from the fault

### Conditions for Clearing the DTC

• | A current DTC becomes history when conditions for the fault are no longer present and the ignition cycles from OFF to ON.

• | A history DTC will clear after 20 ignition cycles.

• | Using a scan tool.

### Diagnostic Aids

Check for the following conditions if a history or intermittent DTC is indicated:

• | A damaged wiring harness. Inspect the wiring harness for damage. If the wiring harness appears to be in good condition, observe the display on the DMM while moving the connectors and wiring harnesses related to the circuits. A change in the DMM display during this test will indicate the location of the fault.

• | For additional information, refer to Testing for Intermittent Conditions and Poor Connections in Wiring Systems.

### Test Description

The number(s) below refer to the step number(s) on the diagnostic table.

1. This step tests the low control circuit of the auto level control relay K19.

2. This step replaces the ALC sensor.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Automatic Level Control (ALC) Diagnostic System Check? | -- | Go to Step 2 | Go to Automatic Level Control Diagnostic System Check
2 |

1. Disconnect the auto level control relay K19 from the relay box.
2. Turn ON the ignition, with the engine OFF.
3. Measure the voltage between the low control circuit of the auto level control relay K19 and ground.

Is the voltage near the specified range?

12 V

Go to Step 3

Go to Step 4

3 | Repair a short to B+ in the low control circuit of the auto level control relay K19. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Step 5 | --
4 | Replace the ALC sensor. Refer to Automatic Level Control Sensor Replacement . Is the repair complete? | -- | Go to Step 5 | --
5 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Step 2