For 1990-2009 cars

### Removal Procedure

1. Remove the disc brake caliper bolts (2). Refer to Rear Brake Caliper Replacement .
2. Lightly wire brush all brake pad contact areas in order to remove any corrosion.

• | Binding

• | Seizing

• | Looseness in the caliper mounting

• | Bent or damaged caliper pins

• | Bent or damaged caliper mounting

3. Ensure the disc brake pads are held firmly in place on the caliper mounting, yet slide easily on the mounting hardware without binding.

### Installation Procedure

1. Install the disc brake caliper & bolts (2). Refer to Rear Brake Caliper Replacement
2. Apply and release the brake pedal (3/4 stroke) as many times as necessary in order to obtain a firm brake pedal.