For 1990-2009 cars

### Removal Procedure

Important: The retainer does not separate from bolster.

1. Remove threaded retainers counterclockwise.
2. Slide bolster down and remove from mounting pins.

### Installation Procedure

1. Position the bolster onto mounting pins and slide up into position and hold.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the threaded retainers clockwise until seated.

Tighten
Tighten the retainers to 2 N·m (18 lb in).