For 1990-2009 cars

### Removal Procedure

The front headrest restraints are not serviceable.

1. Raise the headrest restraint to the full upright position and push in on the tab.
2. Remove the headrest restraint from seat back.

### Installation Procedure

1. Install the headrest restraint to seat back and push in to the full-down position.
2. Raise the headrest restraint to ensure restraint stops at detent.
3. Install the headrest restraint to original position.