For 1990-2009 cars

### Removal Procedure

1. Remove the front console compartment tray and the lid. Refer to Front Floor Console Compartment Replacement
2. Remove the rear vent housing screws from front floor upper console.
3. Remove the separate rear vent housing from front floor upper and lower console.
4. Remove the harness connectors from lighter and switches.
5. Remove the rear heated seat switch panel from rear vent housing.

### Installation Procedure

1. Install the rear heated seat switch panel to rear vent housing.
2. Install the harness connectors to lighter and switches.
3. Install the mount rear vent housing onto front floor upper and lower console.
4. Install the rear vent housing screws to rear vent housing.

Tighten
Tighten the rear vent housing screws until fully seated but not stripped.

5. Install the front console tray and lid. Refer to Front Floor Console Compartment Replacement