For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Using a transmission jack support the rear axle cradle at the differential.
3. Scribe a reference mark on the vehicle body around the perimeter of the rear axle cradle mount to ensure proper installation.
4. Remove the rear axle cradle mount to the vehicle body bolts.
5. Slightly lower the rear axle cradle.
6. Remove the rear axle cradle mount protective shield.
7. Remove the stabilizer shaft link bolts from the lower control arm.
8. Remove the stabilizer shaft link from the lower control arm.
9. Lower the rear cradle.
10. Remove the bolts for the stabilizer shaft mounting brackets.
11. Remove the stabilizer shaft.
12. Transfer stabilizer shaft links. Refer to Stabilizer Shaft Link Replacement .

### Installation Procedure

1. Install the stabilizer shaft.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts for the stabilizer shaft mounting brackets.

Tighten
Tighten the stabilizer shaft mounting bracket bolts to 22 N·m (16 lb ft).

3. Raise the rear axle cradle.
4. Install the stabilizer shaft link to the lower control arm.
5. Install the stabilizer shaft link bolts from the lower control arm.

Tighten
Tighten the stabilizer shaft link bolts to 20 N·m (15 lb ft).

6. Install the rear axle cradle mount protective shields.
7. Raise the rear axle cradle into position.
8. Install the rear axle cradle mount to the vehicle body bolts.

Tighten
Tighten the rear axle cradle mount bolts to 65 N·m (48 lb ft).

9. Remove the transmission jack from the rear differential.
10. Lower the vehicle.
11. Adjust the rear toe to specifications. Refer to Rear Toe Adjustment in Wheel Alignment.