For 1990-2009 cars

### Removal Procedure

1. Remove the rubber conduit from the center pillar:

• | Hold at the center pillar base or at the lower door.

• | Stay close to the ends while using a turning-pulling motion in order to loosen the conduit.

• | Remove the conduit.

2. Disconnect the conduit connectors.
3. Remove the conduit from the wiring harness.

### Installation Procedure

1. Install the conduit on the harnesses.
2. Connect the connectors.
3. Install the conduit to the center pillar.