For 1990-2009 cars

#### Tools Required

J 43301 Coil Pack Remover

### Removal Procedure

1. Relieve the fuel system pressure.

Important: Counterhold the fuel hose connections when loosening to prevent damage to the fuel rail.

2. Disconnect the fuel rail supply and return lines.
3. Unclip and reposition the heater hoses from the retainer.
4. Remove the heater hose retainer bracket bolt from the intake plenum.
5. Remove the heater hose retainer bracket.
6. Disconnect the coil pack electrical connector.
7. Remove the coil pack retainer bolts.

Important: DO NOT overtighten the J 43301 .

8. Thread the J 43301 into the coil pack.
9. With even pressure, lift and remove the coil pack.
10. Remove the coil pack.

### Installation Procedure

1. Inspect the coil pack seals and spark plug boots for damage or wear.

Replace as necessary.

2. Align the spark plug boots with the spark plugs.
3. Carefully press and seat the coil pack in place.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the coil pack retainer bolts.

Tighten
Tighten the coil pack retainer bolts to 8 N·m (71 lb in).

5. Connect the coil pack electrical connector.
6. Install the heater hose retainer bracket to the intake plenum.
7. Install the heater hose retainer bracket bolt.

Tighten
Tighten the heater hose retainer bracket bolt to 8 N·m (71 lb in).

8. Install and secure the heater hoses to the retainer.

Important: Counterhold the fuel hose connections when tightening to prevent damage to the fuel rail.

9. Connect the fuel rail supply and return lines.

Tighten
Tighten the lines to 15 N·m (11 lb ft).