For 1990-2009 cars

Name | Hydra-matic 4L30-E
--- | ---
Production Location | Strasbourg, France
Vehicle Platform (Engine/Transmission) Usage | V
Transmission Drive | Longitudinal Mounted Rear Wheel Drive
Maximum Engine Torque | 350N·m 258 lb ft
1st Gear Ratio | 2.40:1
2nd Gear Ratio | 1.47:1
3rd Gear Ratio | 1.000:1
4th Gear Ratio | 0.72:1
Reverse | 2.00:1
Maximum Shift Speed | 6,500 rpm
Torque Converter Size (Diameter of Torque Converter Turbine) | 245 mm 258 mm 265 mm
Pressure Taps | Line Pressure
Transmission Fluid Type | Dexron™ III
Transmission Fluid Capacity (Approximate) | Dry: 6.4 L (7 qts)
Transmission Type: 4 | Four Forward Gears
Transmission Type: L | Longitudinal Mount
Product Series | 30
Transmission Type: E | Electronic Controls
Position Quadrant | P, R, N, D, 3, 2, 1
Case Material | Die Cast Aluminum
Transmission Weight Dry | 69.1 kg (152 lbs)
Transmission Weight Wet | 76.0 kg (167 lbs)
Maximum Gross Vehicle Weight (GVW) | 3500 kg (7,716 lbs)