For 1990-2009 cars

Table 1: | Inline Connector C100
Table 2: | Inline Connector C101
Table 3: | Inline Connector C102
Table 4: | Inline Connector C105
Table 5: | Inline Connector C106
Table 6: | Inline Connector C108
Table 7: | Inline Connector C110
Table 8: | Inline Connector C111
Table 9: | Inline Connector C112
Table 10: | Inline Connector C200A
Table 11: | Inline Connector C200B
Table 12: | Inline Connector C205
Table 13: | Inline Connector C207 (with side airbags)
Table 14: | Inline Connector C208 (with side airbags)
Table 15: | Inline Connector C209 (with side airbags)
Table 16: | Inline Connector C210
Table 17: | Inline Connector C301
Table 18: | Inline Connector C302
Table 19: | Inline Connector C303
Table 20: | Inline Connector C304
Table 21: | Inline Connector C305
Table 22: | Inline Connector C310
Table 23: | Inline Connector C320
Table 24: | Inline Connector C400
Table 25: | Inline Connector C401
Table 26: | Inline Connector C405
Table 27: | Inline Connector C500
Table 28: | Inline Connector C600

#### Inline Connector C100

Connector Part Information |

• | 12059472

• | ASM 7F M/P MIXED (BLACK)

Connector Part Information

• | 12052200

• | ASM 7M M/PMIXED (BLACK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | GRY/RED | RA1 | RH cornering lamp signal | A | GRY/RED | RA998 | RH cornering lamp signal
B | BLK/WHT | FM1 | LH park/turn lamp signal | B | BLK/WHT | FM40 | LH park/turn lamp signal
C | BLK/GRN | FU1 | RH park/turn lamp signal | C | BLK/GRN | FU40 | RH park/turn lamp signal
D | GRY/BLK | RF1 | LH cornering lamp signal | D | GRY/BLK | RF998 | LH cornering lamp signal
E | BLK | F1 | Ground to G103 | E | BLK | F400 | Ground to G103
F | GRY/GRN | RU1 | B+ from fuse #26 | F | GRY/GRN | RU40 | B+ from fuse #26
G | BRN | X1 | Fog lamp On signal | G | BLK/BLU | FP27 | Fog lamp On signal

#### Inline Connector C101

Connector Part Information |

• | ZFW 6-3

• | 6 Way F

Connector Part Information

• | ZMW 6-3

• | 6 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | RED | A990 | B+ from fuse #33 | 1 | RED | A2 | B+ from fuse #33
2 | BLU | P50 | MIL request output signal | 2 | BLU | P390 | MIL request output signal
3 | YEL/BLU | BP900 | A/C cutout signal | 3 | YEL/BLU | BP1 | A/C cutout signal
4 | BLK/WHT | FM7 | A/C request signal | 4 | BLK/WHT | FM7 | A/C request signal
5 | BRN | X79 | B+ from fuse #13 | 5 | BRN | X69 | B+ from fuse #13
6 | -- | -- | NOT USED | 6 | -- | -- | NOT USED

#### Inline Connector C102

Connector Part Information |

• | ZFW 6-4

• | 6 Way F

Connector Part Information

• | ZMW 6-4

• | 6 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
2 | BLU/GRN | PU1 | Oil pressure switch signal | 2 | BLU/GRN | PU1 | Oil pressure switch signal
3 | BLU/WHT | PM1 | Charging indicator signal | 3 | BLU/WHT | PM1 | Charging indicator signal
4 | BRN/GRN | XU4 | Oil level signal | 4 | BRN/GRN | XU600 | Oil level signal
5 | -- | -- | NOT USED | 5 | -- | -- | NOT USED
6 | BLK | F120 | Oil level signal | 6 | BLK | F63 | Oil level signal
8 | BLK/RED | FA50 | Starter switch signal | 8 | BLK/RED | FA501 | Starter switch signal
14 | BLU/YEL | PB1 | Oil pressure sensor signal | 14 | BLU/YEL | PB90 | Oil pressure sensor signal

#### Inline Connector C105

Connector Part Information |

• | ZFW 20-2

• | 20 Way F

Connector Part Information

• | ZMW 20-2

• | 20 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP770 | B+ from fuel pump relay | 1 | RED/BLU | AP77 | B+ from fuel pump relay
2 | BRN | X68 | B+ to ignition coil | 2 | BRN | X68 | B+ to ignition coil
3 | BRN/WHT | XM88 | Serial data | 3 | BRN/WHT | XM100 | Serial data
4 | -- | -- | NOT USED | 4 | -- | -- | NOT USED
5 | BRN/BLU | XP8 | MIL control signal | 5 | BRN/BLU | XP22 | MIL control signal
6 | WHT/BLK | MF757 | Transmission position signal | 6 | WHT/BLK | MF757 | Transmission position signal
7 | BLU/RED | PA79 | Vehicle speed signal | 7 | BLU/RED | PA14 | Vehicle speed signal
8 | BRN | X756 | B+ from fuse #3 | 8 | BRN | X757 | B+ from fuse #3
9 | -- | -- | NOT USED | 9 | -- | -- | NOT USED
10 | BRN/YEL | XB82 | TPS output signal | 10 | BRN/YEL | XB54 | TPS output signal
11 | BLU | P900 | Coolant temperature signal | 11 | BLU | P900 | Coolant temperature signal
12 | BLU/BLK | PF73 | Fuel level signal | 12 | BLU/BLK | PF10 | Fuel level signal
13 | GRN | U80 | Tachometer output signal | 13 | GRN | U744 | Tachometer output signal
14 | GRY | R48 | Engine torque input signal | 14 | GRY | R38 | Engine torque input signal
15 | BRN | X56 | Ignition positive voltage | 15 | BRN | X128 | Ignition positive voltage
16 | BRN/YEL | XB72 | Fuel pressure sensor signal | 16 | BRN/YEL | XB900 | Fuel pressure sensor signal
17 | BLU/BLK | PF532 | 5V reference | 17 | BLU/BLK | PF900 | 5V reference
18 | BRN/GRN | XU718 | Sensor ground | 18 | BRN/GRN | XU900 | Sensor ground
19 | GRY | R83 | Engine torque output signal | 19 | GRY | R800 | Engine torque output signal
20 | -- | -- | NOT USED | 20 | -- | -- | NOT USED

#### Inline Connector C106

Connector Part Information |

• | ZFW 20-2

• | 20 Way F

Connector Part Information

• | ZMW 20-2

• | 20 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BLK/RED | FA500 | Positive ignition voltage | 1 | BLK/RED | FA700 | positive ignition voltage
2 | BLK/RED | FA501 | Transmission position signal | 2 | BLK/RED | FA501 | Transmission position signal
3 | BLU/YEL | PB743 | 2-3 shift solenoid control | 3 | BLU/YEL | PB743 | 2-3 shift solenoid control
4 | GRY/BLK | RF745 | Brake band signal | 4 | GRY/BLK | RF745 | Brake band signal
5 | BLU/BLK | PF754 | Common | 5 | BLU/BLK | PF754 | Common
6 | BLU/WHT | PM748 | 1-2 and 3-4 shift solenoid control | 6 | BLU/WHT | PM748 | 1-2 and 3-4 shift solenoid control
7 | BLK/YEL | FB738 | TCC solenoid control | 7 | BLK/YEL | FB738 | TCC solenoid control
8 | BLK/PPL | FY740 | Pressure control solenoid signal | 8 | BLK/PPL | FY740 | Pressure control solenoid control
9 | BLK/BLU | FP722 | Transmission fluid temperature signal | 9 | BLK/BLU | FP722 | Transmission fluid temperature signal
10 | GRY/RED | RA741 | Pressure control solenoid signal | 10 | GRY/RED | RA741 | Pressure control solenoid signal
11 | BLU/GRN | PU705 | Output shaft speed signal | 11 | BLU/GRN | PU714 | Output shaft speed signal
12 | BLK | S10 | Shield wire | 12 | BLK | S40 | Shield wire
13 | BRN/GRN | XU21 | Torque control input | 13 | BRN/GRN | XU51 | Torque control input
14 | BLK/YEL | FB708 | Transmission position signal | 14 | BLK/YEL | FB708 | Transmission position signal
15 | BLK/YEL | FB703 | Output shaft speed signal | 15 | BLK/YEL | FB720 | Output shaft speed signal
16 | BLK/RED | FA69 | P/N input | 16 | BLK/RED | FA701 | P/N input
17 | GRY | R733 | Transmission position signal | 17 | GRY | R733 | Transmission position signal
18 | BLK/BLU | FP723 | Transmission position signal | 18 | BLK/BLU | FP10 | Transmission position signal
19 | BLK/GRN | FU726 | Transmission position signal | 19 | BLK/GRN | FU2 | Transmission position signal
20 | BRN/GRN | XU716 | Transmission fluid temperature signal | 20 | BRN/GRN | XU716 | Transmission fluid temperature signal

#### Inline Connector C108

Connector Part Information |

• | ZPF 2-3

• | 2 Way F

Connector Part Information

• | ZPM 2-3

• | 2 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BRN | X1 | Heated nozzle On signal | A | BRN | X600 | Heated nozzle On signal
B | BLK | F1 | Ground to G103 | B | BLK | F600 | Ground to G103

#### Inline Connector C110

Connector Part Information |

• | ZF 9-22

• | 9 Way F

Connector Part Information

• | ZM 9-22

• | 9 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PPL | Y370 | Secondary air injection pump control | 1 | BRN/GRN | XR200 | Secondary air injection pump control
2 | BLK/BLU | FP120 | A/C request signal | 2 | BLK/BLU | FP99 | A/C request signal
3 | PPL | Y67 | Secondary air injection pump valve control | 3 | BRN/YEL | XB900 | Secondary air injection pump valve control
4 | BLK/WHT | FM430 | A/C request input | 4 | BLK/WHT | FM99 | A/C request input
5 | BRN/PPL | XY360 | A/C compressor relay control | 5 | BRN/PPL | XY107 | A/C compressor relay control
6 | RED/BLU | AP960 | B+ from relay K43 | 6 | RED/BLU | AP200 | B+ from relay K43
7 | BLU | P390 | MIL input signal | 7 | BLU | P390 | MIL input signal
8-9 | -- | -- | NOT USED | 8-9 | -- | -- | NOT USED

#### Inline Connector C111

Connector Part Information |

• | ZFW 6-3

• | 6 Way F

Connector Part Information

• | ZMW 6-3

• | 6 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BRN | X68 | B+ from fuse #10 | 1 | BRN | X67 | B+ from fuse #10
2 | BLK/YEL | FB1 | Interval switch signal | 2 | BLK/YEL | FB3 | Interval switch signal
3 | BLU | P2 | Windshield washer relay signal | 3 | BLU | P2 | Windshield washer relay signal
4 | GRN | U10 | Windshield washer motor signal | 4 | GRN | U6 | Windshield washer motor signal
5 | BLK/RED | FA1 | Windshield washer pump signal | 5 | BLK/RED | FA5 | Windshield washer pump signal
6 | BLK/PPL | FY1 | B+ from fuse #9 | 6 | BLK/PPL | FY3 | B+ from fuse #9

#### Inline Connector C112

Connector Part Information |

• | 12059472

• | ASM 7F M/P MIXED (BLACK)

Connector Part Information

• | 12052200

• | ASM 7M M/P MIXED (BLACK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BRN/YEL | XB17 | Fuel injector #1 control | A | BRN/YEL | XB17 | Fuel injector #1 control
B | BRN/GRN | XU16 | Fuel injector #2 control | B | BRN/GRN | XU16 | Fuel injector #2 control
C | BRN/BLU | XP35 | Fuel injector #3 control | C | BRN/BLU | XP35 | Fuel injector #3 control
D | BRN/RED | XA34 | Fuel injector #4 control | D | BRN/RED | ZA34 | Fuel injector #4 control
E | BRN/BLK | XF15 | Fuel injector #5 control | E | BRN/BLK | XF15 | Fuel injector #5 control
F | BRN/PPL | XY33 | Fuel injector #6 control | F | BRN/PPL | XY33 | Fuel injector #6 control
G | RED/BLU | AP751 | B+ from relay K43 | G | RED/BLU | AP751 | B+ from relay K43

#### Inline Connector C200A

Connector Part Information |

• | ZF 62-1

• | 62 Way F

Connector Part Information

• | ZM 62-1

• | 62 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BLK/YEL | FB10 | B+ to auxiliary brake lamp | 1 | BLK/YEL | FB303 | B+ to auxiliary brake lamp
2 | BLU/BLK | PF1 | Fuel gauge level signal | 2 | BLU/BLK | PF12 | Fuel gauge level signal
3 | RED | A701 | B+ from fuse #25 | 3 | RED | A700 | B+ from fuse #25
4 | BRN/WHT | XM2 | Park brake indicator | 4 | BRN/WHT | XM2 | Park brake indicator
5 | BLK/BLU | FP36 | B+ when fog lamps are ON | 5 | BLK/BLU | PF27 | B+ when fog lamps are ON
6 | BLK/GRN | FU11 | RH turn and taillamp signal | 6 | BLK/GRN | FU1 | RH turn and taillamp signal
7 | BLK/WHT | FM12 | LH turn and taillamp signal | 7 | BLK/WHT | FM1 | LH turn and taillamp signal
8 | GRY/WHT | RM1 | Interior lamps ON/OFF signal | 8 | GRY/WHT | RM1 | Interior lamps ON/OFF signal
9 | BRN/PPL | XY800 | Delayed interior relay signal | 9 | BRN/PPL | XY800 | Delayed interior relay signal
10 | RED/BLU | AP807 | Rear compartment open signal | 10 | RED/BLU | AP822 | Rear compartment open signal
11 | BRN/WHT | XM42, XM43 | RH rear door speaker return | 11 | BRN/WHT | XM42 | RH rear door speaker return
12 | RED | A48 | B+ from fuse #1 | 12 | RED | A10 | B+ from fuse #1
13 | BRN/BLK | XF830 | TWS indicator | 13 | BRN/BLK | XF830 | TWS indicator
14 | BRN/BLU | XP840 | Security lamp indicator | 14 | BRN/BLU | XP840 | Security lamp indicator
15 | BRN | X15 | B+ when defogger is ON | 15 | BRN | X16 | B+ when defogger is ON
16 | GRY/GRN | RU10 | B+ when park lamps are ON | 16 | GRY/GRN | RU7 | B+ when park lamps are ON
17 | BRN/WHT | XM600 | Serial data | 17 | BRN/WHT | XM830 | Serial data
18 | BLK/BRN | FX810 | TWS delay signal | 18 | BLK/BRN | FX810 | TWS delay signal
19 | BRN/BLU | XP803 | Low when interior lamps are ON | 19 | BRN/BLU | XP803 | Low when interior lamps are ON
20 | BRN/PPL | XY112 | Interior lamps ON/OFF signal | 20 | BRN/PPL | XY112 | Interior lamps ON/OFF signal
21 | BRN/GRN | XU42, XU43 | LH rear door speaker return | 21 | BRN/GRN | XU42 | LH rear door speaker return
22 | BRN/YEL | XB10, XB12 | RH front door speaker return | 22 | BRN/YEL | XB10 | RH front door speaker return
23 | GRN | U41, U42 | LH rear door speaker feed | 23 | GRN | U42 | LH rear door speaker feed
24 | BRN/BLU | XP4, XP5 | LH front door speaker return | 24 | BRN/BLU | XP1 | LH front door speaker return
25 | YEL | B8, B9 | RH front door speaker feed | 25 | YEL | B10 | RH front door speaker feed
26 | BLU | P1, P5 | LH front door speaker feed | 26 | BLU | P1 | LH front door speaker feed
27 | BRN/WHT | XM30 | Horn relay control signal | 27 | BRN/WHT | XM70 | Horn relay control signal
28 | BLK/RED | FA3 | WSWA pump signal | 28 | BLK/RED | FA80 | WSWA pump signal
29 | -- | -- | NOT USED | 29 | -- | -- | NOT USED
30 | BRN/YEL | XB3 | WSWA solvent level indicator signal | 30 | BRN/YEL | XB3 | WSWA solvent level indicator signal
31 | YEL/RED | BA2 | Brake wear sensor signal | 31 | YEL/RED | BA2 | Brake wear sensor signal
32 | BLU/WHT | PM4 | Outside temperature signal | 32 | BLU/WHT | PM4 | Outside temperature signal
33 | BRN | X79 | B+ from fuse #13 | 33 | BRN | X999 | B+ from fuse #13
34 | BLU | P11 | Ground | 34 | BLU | P11 | Ground
35 | BRN/WHT | XM700 | Serial data | 35 | BRN/WHT | XM700 | Serial data
36 | WHT/BLK | MF757 | B+ with automatic transmission range switch in reverse | 36 | WHT/BLK | MF10, MF900 | B+ with automatic transmission range switch in reverse
37 | RED/WHT | AM813 | Low when park lamps are ON | 37 | RED/WHT | AM899 | Low when park lamps are ON
38 | BLK/PPL | FY810 | TWS return | 38 | BLK/PPL | FY810 | TWS return
39 | BRN/WHT | XM999 | Serial data | 39 | BRN/WHT | XM55 | Serial data
40 | WHT | M42, M43 | RH rear door speaker feed | 40 | WHT | M42 | RH rear door speaker feed
41 | BRN/BLK | XF20 | Seat belt warning signal | 41 | BRN/BLK | XF21 | Seat belt warning signal
42 | RED/WHT | AM110 | Radio ON signal | 42 | RED/WHT | AM42 | Radio ON signal
43 | BRN/YEL | XB4 | ABS indicator signal | 43 | BRN/YEL | XB305 | ABS indicator signal
44 | RED | A24 | B+ from fuse #4 | 44 | RED | A6 | B+ from fuse #4
45 | BRN/YEL | XB105 | ABS indicator signal | 45 | BRN/YEL | XB105 | ABS indicator signal
46 | BLU/RED | PA10 | Vehicle speed signal | 46 | BLU/RED | PA901, PA909 | Vehicle speed signal
47 | RED | A49 | B+ from fuse #7 | 47 | RED | A2 | B+ from fuse #7
48 | RED | A816 | B+ from fuse #28 | 48 | RED | A13, A823 | B+ from fuse #28
49 | BRN | X300 | B+ from fuse #15 | 49 | BRN | X100 | B+ from fuse #15
50 | RED | A65 | B+ from fuse #35 | 50 | RED | A65 | B+ from fuse #35
96 | YEL | B11 | B+ when low beams are ON | 96 | YEL | B1 | B+ when low beams are ON
97 | GRY/YEL | RB200 | Dimmer signal | 97 | GRY/YEL | RB200 | Dimmer signal
98 | WHT | M64 | B+ when high beams are ON | 98 | WHT | M1 | B+ when high beams are ON
99 | BLK/RED | FA202 | B+ from fuse #19 | 99 | BLK/RED | FA202 | B+ from fuse #19
100 | YEL | B22 | B+ when low beams are ON | 100 | YEL | B3 | B+ when low beams are ON
101 | BRN/PPL | XY801 | Interior lamps relay signal | 101 | BRN/PPL | XY801 | Interior lamps relay signal
102 | GRY/RED | RA30 | B+ when park lamps are ON | 102 | GRY/RED | RA2 | B+ when park lamps are ON
103 | GRY/BLK | RF30 | B+ when park lamps are ON | 103 | GRY/BLK | RF2 | B+ when park lamps are ON
104 | BRN/YEL | XB910 | HEADLAMPS ON REQUIRED signal | 104 | BRN/YEL | XB910 | HEADLAMPS ON REQUIRED signal
105 | BRN/WHT | XM300 | Serial data | 105 | BRN/WHT | XM218 | Serial data
106 | BLK/WHT | FM100 | B+ from fuse #11 | 106 | BLK/WHT | FM10, FM22 | B+ from fuse #11
107 | RED | A301 | B+ from fuse #17 | 107 | RED | A30 | B+ from fuse #17

#### Inline Connector C200B

Connector Part Information |

• | ZF 45-2

• | 45 Way F

Connector Part Information

• | ZM 45-2

• | 45 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
51 | BLK/RED | FA811 | Fuel door release signal | 51 | BLK/RED | FA811 | Fuel door release signal
52 | YEL | B56 | ALC relay control signal | 52 | YEL | B25 | ALC relay control signal
53 | RED/WHT | AM810 | Low when park lamps are ON | 53 | RED/WHT | AM810 | Low when park lamps are ON
54 | GRY | R38, R40 | Engine torque request | 54 | GRY | R40 | Engine torque request
55 | BRN/PPL | XY2 | Leveling indicator signal | 55 | BRN/PPL | XY1 | Leveling indicator signal
56 | BRN/WHT | XM900 | Serial data | 56 | BRN/WHT | XM900 | Serial data
57 | BRN/BLU | XP810 | Battery guard signal | 57 | BRN/BLU | XP811 | Battery guard signal
58 | RED | A892 | Low when high beams are ON | 58 | RED | A810, A888 | Low when high beams are ON
59 | BRN/WHT | XM810 | Low when park lamps are ON | 59 | BRN/WHT | XM810 | Low when park lamps are ON
60 | BRN/RED | XA810 | Low beam relay signal | 60 | BRN/RED | XA810 | Low beam relay signal
61 | WHT | M8 | B+ when high beams are ON | 61 | WHT | M2 | B+ when high beams are ON
62 | BRN/RED | XA105 | Traction control ON signal | 62 | BRN/RED | XA105 | Traction control ON signal
63 | BLK/WHT | FM19 | LH high beam headlamp signal | 63 | BLK/WHT | FM13 | LH high beam headlamp signal
64 | BLK/YEL | FB7 | Seat heater ON signal | 64 | BLK/YEL | FB7 | Seat heater ON signal
65 | BLK/RED | FA9 | Seat heater ON signal | 65 | BLK/RED | FA9 | Seat heater On signal
66 | BRN/WHT | XM899 | Horn relay control signal | 66 | BRN/WHT | XM899 | Horn relay control signal
67 | GRY/RED | RA999 | B+ to RH cornering lamp | 67 | GRY/RED | RA998 | B+ to RH cornering lamp
68 | GRY/BLK | RF999 | B+ to LH cornering lamp | 68 | GRY/BLK | RF998 | B+ to LH cornering lamp
69 | RED | A12, A900 | B+ from fuse #24 | 69 | RED | A999 | B+ from fuse #24
70 | BLK/RED | FA812 | Rear compartment lid release signal | 70 | BLK/RED | FA812, XY900 | Rear compartment lid release signal
71 | WHT | M3 | High beams ON/OFF signal | 71 | WHT | M50 | High beams ON/OFF signal
72 | PPL | Y40 | Actual transmission torque | 72 | PPL | Y40 | Actual transmission torque
73 | BRN/YEL | XB900 | Fuel pressure sensor signal | 73 | BRN/YEL | XB902 | Fuel pressure sensor signal
74 | BRN/GRN | XU900 | Sensor ground | 74 | BRN/GRN | XU900 | Sensor ground
75 | BLK/RED | FA825 | Brake to shift indicator | 75 | BLK/RED | FA399 | Brake to shift indicator
76 | YEL | B900 | Gear out of park signal | 76 | YEL | B900 | Gear out of park signal
77 | RED | A101 | B+ from fuse #27 | 77 | RED | A295 | B+ from fuse #27
78 | RED/BLU | AP4 | B+ from fuse #18 | 78 | RED/BLU | AP11 | B+ from fuse #18
79 | BRN | X43 | ALC compressor motor signal | 79 | BRN | X101 | ALC compressor motor signal
80 | BRN | X6 | B+ from fuse #14 | 80 | BRN | X6 | B+ from fuse #14
81 | RED/YEL | AB810 | TWS ON/OFF signal | 81 | RED/YEL | AB810 | TWS ON/OFF signal
82 | -- | -- | NOT USED | 82 | -- | -- | NOT USED
83 | GRY | R800, R802 | Engine torque signal | 83 | GRY | R830 | Engine torque signal
84 | BRN/BLU | XP900 | Rear compartment lid release open indicator | 84 | BRN/BLU | XP901 | Rear compartment lid release open indicator
85 | WHT | M69, M75 | High beams ON signal | 85 | WHT | M60 | High beams ON signal
86 | YEL | B60 | Low beam ON/OFF signal | 86 | YEL | B899 | Low beam ON/OFF signal
87 | BRN | X67, X838 | B+ from fuse #10 | 87 | BRN | X826 | B+ from fuse #10
88 | BRN/PPL | XY802 | Low when high beams are ON | 88 | BRN/PPL | XY802 | Low when high beams are ON
89 | BLU/BLK | PF900 | 5V reference | 89 | BLU/BLK | PF901 | 5V reference
90 | BRN/BLU | XP33 | TWS day/night signal | 90 | BRN/BLU | XP830 | TWS day/night signal
91 | WHT | M808 | Fast wiper signal | 91 | WHT | M808 | Fast wiper signal
92 | GRN | U50 | Tachometer output signal | 92 | GRN | U102 | Tachometer output signal
93 | BLK/BRN | FX750 | Stoplamp switch signal | 93 | BLK/BRN | FX899 | Stoplamp switch signal
94 | YEL | B810 | Wiper 1 interval signal | 94 | YEL | B810 | Wiper 1 interval signal

#### Inline Connector C205

Connector Part Information |

• | F 9-23

• | 9 Way F

Connector Part Information

• | M 9-23

• | 9 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | GRN | U900 | Lifting magnet control signal | 1 | -- | -- | Lifting magnet control signal
2 | BLU | P100 | Second gear start signal | 2 | -- | -- | Second gear start signal
3-5 | -- | -- | NOT USED | 3-5 | -- | -- | NOT USED
6 | BLK | F950, F960 | Ground to G103 | 6 | -- | -- | Ground to G103
7 | YEL | B901 | Ground supply for fuel tank filler release switch | 7 | -- | -- | Ground supply for fuel tank filler release switch
8 | BLK/BRN | FX900 | B+ when stop lamp switch is closed | 8 | -- | -- | B+ when stop lamp switch is closed
9 | YEL | B900 | Gear out of park signal to BCM | 9 | -- | -- | Gear out of park signal to BCM

#### Inline Connector C207 (with side airbags)

Connector Part Information |

• | ZF 9-34

• | 9 Way F

Connector Part Information

• | ZM 9-34

• | 9 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BRN/YEL | XB950 | Passenger seat pretensioner signal LOW | 1 | BRN/YEL | XB901 | Passenger seat pretensioner signal LOW
2 | RED/YEL | AB950 | Passenger seat pretensioner signal HIGH | 2 | RED/YEL | AB900 | Passenger seat pretensioner signal HIGH
3 | RED/WHT | AM950 | Driver seat pretensioner signal HIGH | 3 | RED/WHT | AM900 | Driver seat pretensioner signal HIGH
4 | BRN/WHT | XM950 | Driver seat pretensioner signal LOW | 4 | BRN/WHT | XM901 | Driver seat pretensioner signal LOW
5 | YEL | B41 | Driver seat side impact sensor signal | 5 | YEL | B41 | Driver seat side impact sensor signal
6 | BRN/YEL | XB42 | Driver seat side impact sensor signal | 6 | BRN/YEL | XB42 | Driver seat side impact sensor signal
7 | BRN/WHT | XM430 | Passenger seat side impact sensor signal | 7 | BRN/WHT | XM430 | Passenger seat side impact sensor signal
8 | WHT | M44 | Passenger seat side impact sensor signal | 8 | WHT | M44 | Passenger seat side impact sensor signal
9 | BRN/PPL | XY999 | ONSTAR signal | 9 | BRN/PPL | XY999 | ONSTAR signal

#### Inline Connector C208 (with side airbags)

Connector Part Information |

• | ZF 2-15

• | 2 Way F

Connector Part Information

• | ZM 2-15

• | 2 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | RED/YEL | AB11 | Driver side HIGH signal | 1 | RED/YEL | AB11 | Driver side HIGH signal
2 | BRN/YEL | XB100 | Driver side LOW signal | 2 | BRN/YEL | XB100 | Driver side LOW signal

#### Inline Connector C209 (with side airbags)

Connector Part Information |

• | ZF 2-16

• | 2 Way F

Connector Part Information

• | ZM 2-16

• | 2 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | RED/WHT | AM13 | Passenger side HIGH signal | 1 | RED/WHT | AM13 | Passenger side HIGH signal
2 | BRN/WHT | XM14 | Passenger side LOW signal | 2 | BRN/WHT | XM14 | Passenger side LOW signal

#### Inline Connector C210

Connector Part Information |

• | ZF 42-3

• | 42 Way F

Connector Part Information

• | ZM 42-3

• | 42 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | RED | A202 | B+ from fuse #6 | 1 | RED | A200 | B+ from fuse #6
2 | BLK | F102 | Ground to G201 | 2 | BLK | F100 | Ground to G201
3 | BRN/WHT | XM160 | Serial data | 3 | BRN/WHT | XM15 | Serial data
4 | BRN/WHT | XM45 | Serial data | 4 | BRN/WHT | XM45 | Serial data
5 | BLK | S45 | Shield wire | 5 | BLK | S45 | Shield wire
6 | WHT | M90 | Sound processor signal | 6 | WHT | M90 | Sound processor signal
7 | BRN/WHT | XM93 | Sound processor signal | 7 | BRN/WHT | XM90 | Sound processor signal
8 | BLK | S46 | Shield wire | 8 | BLK | S46 | Shield wire
9 | WHT | M91 | Sound processor signal | 9 | WHT | M91 | Sound processor signal
10 | BRN/WHT | XM91 | Sound processor signal | 10 | BRN/WHT | XM91 | Sound processor signal
11 | BLK | S47 | Shield wire | 11 | BLK | S47 | Shield wire
12 | WHT | M92 | Sound processor signal | 12 | WHT | M92 | Sound processor signal
13 | BRN/WHT | XM92 | Sound processor signal | 13 | BRN/WHT | XM92 | Sound processor signal
14 | BRN/WHT | XM43 | RH rear door speaker signal | 14 | BRN/WHT | XM43 | RH rear door speaker signal
15 | WHT | M43 | RH rear door speaker signal | 15 | WHT | M43 | RH rear door speaker signal
16 | BRN/BLU | XP5 | LH front door speaker signal | 16 | BRN/BLU | XP2 | LH front door speaker signal
17 | BLU | P5 | LH front door speaker signal | 17 | BLU | P2 | LH front door speaker signal
18 | BRN/YEL | XB12 | RH front door speaker signal | 18 | BRN/YEL | XB11 | RH front door speaker signal
19 | RED | A201 | B+ from fuse #8 | 19 | RED | A201 | B+ from fuse #8
20 | BLK | F101 | Ground to G201 | 20 | BLK | F101 | Ground to G201
21 | -- | -- | NOT USED | 21 | -- | -- | NOT USED
22 | YEL | B9 | RH front door speaker signal | 22 | YEL | B4 | RH front door speaker signal
23 | BRN/GRN | XU43 | LH rear door speaker signal | 23 | BRN/GRN | XU43 | LH rear door speaker signal
24 | GRN | U42 | LH rear door speaker signal | 24 | GRN | U43 | LH rear door speaker signal
25 | -- | -- | NOT USED | 25 | -- | -- | NOT USED
26 | YEL | B20 | CD player signal | 26 | YEL | B20 | CD player signal
27-28 | -- | -- | NOT USED | 27-28 | -- | -- | NOT USED
29 | RED | X405 | B+ from fuse #14 | 29 | BRN/YEL | A10 | B+ from fuse #14
30 | BLK | F405 | Ground to G201 | 30 | BLK | F10 | Ground to G201
31 | RED | A405 | B+ from multifunction relay | 31 | RED | A11, A205 | B+ from multifunction relay
32-42 | -- | -- | NOT USED | 32-42 | -- | -- | NOT USED

#### Inline Connector C301

Connector Part Information |

• | F 9-3

• | 9 Way F

Connector Part Information

• | M 9-3

• | 9 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | GRY | R2 | RH rear side door jamb switch signal | 1 | GRY | R18 | RH rear side door jamb switch signal
2 | RED/BLU | AP1 | RH roof rail courtesy lamp signal | 2 | RED/BLU | AP809 | RH roof rail courtesy lamp signal
3 | -- | -- | NOT USED | 3 | -- | -- | NOT USED
4 | BRN/BLU | XP1 | Rear compartment lid open signal | 4 | BRN/BLU | XP805 | Rear compartment lid open signal
5 | -- | -- | NOT USED | 5 | -- | -- | NOT USED
6 | BLK | F1 | Ground to G103 | 6 | BLK | F88 | Ground to G103
7 | -- | -- | NOT USED | 7 | -- | -- | NOT USED
8 | GRY | R1 | RH rear side door jamb switch signal | 8 | GRY | R16 | RH rear side door jamb switch signal
9 | -- | -- | NOT USED | 9 | -- | -- | NOT USED

#### Inline Connector C302

Connector Part Information |

• | F 9-3

• | 9 Way F

Connector Part Information

• | M 9-3

• | 9 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | GRY | R2 | LH rear side door jamb switch signal | 1 | GRY | R18 | LH rear side door jamb switch signal
2 | RED/BLU | AP1 | LH roof rail courtesy lamp signal | 2 | RED/BLU | AP809 | LH roof rail courtesy lamp signal
3 | -- | -- | NOT USED | 3 | -- | -- | NOT USED
4 | BRN/BLU | XP1 | Rear compartment lid open signal | 4 | BRN/BLU | XP805 | Rear compartment lid open signal
5 | -- | -- | NOT USED | 5 | -- | -- | NOT USED
6 | BLK | F1 | Ground to G103 | 6 | BLK | F88 | Ground to G103
7 | -- | -- | NOT USED | 7 | -- | -- | NOT USED
8 | GRY | R1 | LH rear side door jamb switch signal | 8 | GRY | R16 | LH rear side door jamb switch signal
9 | -- | -- | NOT USED | 9 | -- | -- | NOT USED

#### Inline Connector C303

Connector Part Information |

• | ZF15-4

• | 15 Way F

Connector Part Information

• | ZM15-4

• | 15 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | YEL | B7 | Memory programming signal | 1 | YEL | B1 | Memory programming signal
2 | BLK/RED | FA804 | Doors unlock signal | 2 | BLK/RED | FA804 | Doors unlock signal
3 | BLK/YEL | FB805 | Doors lock signal | 3 | BLK/YEL | FB805 | Doors lock signal
4 | BLK | F19 | Ground | 4 | BLK | F3 | Ground
5 | GRY/GRN | RU15 | Window up signal | 5 | GRY/GRN | RU1, RU2 | Window up signal
6-7 | -- | -- | NOT USED | 6-7 | -- | -- | NOT USED
8 | RED | A21 | B+ from fuse #7 | 8 | RED | A1 | B+ from fuse #7
9 | BLU/RED | PA3 | Window down signal | 9 | BLU/RED | PA1, PA2 | Window down signal
10 | WHT | M3 | Rear window switch enable signal | 10 | WHT | M1 | Rear window switch enable signal
11 | GRY | R17 | Ground | 11 | GRY | R1 | Ground
12 | GRN | U42 | Speaker and tweeter feed signal | 12 | GRN | U2, U3 | Speaker and tweeter feed signal
13 | BRN/GRN | XU42 | Speaker and tweeter return signal | 13 | BRN/GRN | XU2, XU3 | Speaker and tweeter return signal
14 | -- | -- | NOT USED | 14 | -- | -- | NOT USED
15 | RED/BLU | AP805 | B+ to rear door lamp | 15 | RED/BLU | AP805 | B+ to rear door lamp

#### Inline Connector C304

Connector Part Information |

• | ZF 15-4

• | 15 Way F

Connector Part Information

• | ZM 15-4

• | 15 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | YEL | B8 | Memory programming signal | 1 | YEL | B1 | Memory programming signal
2 | BLK/RED | FA803 | Doors unlock signal | 2 | BLK/RED | FA804 | Doors unlock signal
3 | BLK/YEL | FB804 | Doors lock signal | 3 | BLK/YEL | FB805 | Doors lock signal
4 | BLK | F18 | Ground | 4 | BLK | F3 | Ground
5 | GRY/GRN | RU16 | Window up signal | 5 | GRY/GRN | RU1, RU2 | Window up signal
6-7 | -- | -- | NOT USED | 6-7 | -- | -- | NOT USED
8 | RED | A11 | B+ from fuse #7 | 8 | RED | A1 | B+ from fuse #7
9 | BLU/RED | PA4 | Window down signal | 9 | BLU/RED | PA1, PA2 | Window down signal
10 | WHT | M4 | Rear window switch enable signal | 10 | WHT | M1 | Rear window switch enable signal
11 | GRY | R18 | Ground | 11 | GRY | R1 | Ground
12 | GRN | M42 | Speaker and tweeter feed signal | 12 | GRN | U2, U3 | Speaker and tweeter feed signal
13 | BRN/GRN | XM42 | Speaker and tweeter return signal | 13 | BRN/GRN | XU2, XU3 | Speaker and tweeter return signal
14 | -- | -- | NOT USED | 14 | -- | -- | NOT USED
15 | RED/BLU | AP804 | B+ to rear door lamp | 15 | RED/BLU | AP805 | B+ to rear door lamp

#### Inline Connector C305

Connector Part Information |

• | ZPF 2-50

• | 2 Way F

Connector Part Information

• | ZPM 2-50

• | 2 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BLK | F2 | Ground to G103 | A | BLK | F900 | Ground to G103
B | RED/BLU | AP2 | Sunshade ON signal | B | RED/BLU | AP803 | Sunshade ON signal

#### Inline Connector C310

Connector Part Information |

• | F 20-1

• | 20 Way F

Connector Part Information

• | M 20-1

• | 20 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | RED | A40 | B+ from fuse #28 | 1 | RED | A40 | B+ from fuse #28
2 | BRN | X13 | B+ from fuse #15 | 2 | BRN | X13 | B+ from fuse #15
3 | BLK | F40 | Ground to G103 | 3 | BLK | F40 | Ground to G103
4 | BRN/WHT | XM55 | Serial data | 4 | BRN/WHT | XM55 | Serial data
5 | GRY/WHT | RM12 | Door open signal | 5 | GRY/WHT | RM12 | Door open signal
6 | BLK/BRN | FX75 | Memory potentiometer signal | 6 | BLK/BRN | FX75 | Memory potentiometer signal
7 | X75 | X75 | Memory potentiometer signal | 7 | BRN | X75 | Memory potentiometer signal
8 | GRY/GRN | RU60 | RH outside rear view mirror memory signal | 8 | GRY/GRN | RU60 | RH outside rear view mirror memory signal
9 | GRY | R70 | RH outside rear view mirror memory signal | 9 | GRY | R70 | RH outside rear view mirror memory signal
10 | GRY/BLK | RF60 | Inside rear view mirror memory signal | 10 | GRY/BLK | RF60 | Inside rear view mirror memory signal
11 | GRY/YEL | RB60 | Inside rear view mirror memory signal | 11 | GRY/YEL | RB60 | Inside rear view mirror memory signal
12 | GRY/GRN | RU50 | Memory potentiometer signal | 12 | GRY/GRN | RU50 | Memory potentiometer signal
13 | GRY | R60 | Memory potentiometer signal | 13 | GRY | R60 | Memory potentiometer signal
14 | BLK/RED | FA75 | RH outside rear view mirror common | 14 | BLK/RED | FA75 | RH outside rear view mirror common
15 | GRN | U80 | LH memory mirror control signal | 15 | GRN | U80 | LH memory mirror control signal
16 | YEL | B12 | LH memory mirror control signal | 16 | YEL | B12 | LH memory mirror control signal
17 | BLU/WHT | PM60 | Inside rear view mirror control signal | 17 | BLU/WHT | PM60 | Inside rear view mirror control signal
18 | BLU/RED | PA60 | Inside rear view mirror control signal | 18 | BLU/RED | PA60 | Inside rear view mirror control signal
19 | BLU | P70 | RH outside rear view mirror control signal | 19 | BLU | P70 | RH outside rear view mirror control signal
20 | GRY | R65 | RH outside rear view mirror control signal | 20 | GRY | R65 | RH outside rear view mirror control signal

#### Inline Connector C320

Connector Part Information |

• | ZF 9-4

• | 9 Way F

Connector Part Information

• | ZM 9-4

• | 9 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | RED | A1 | B+ from fuse #4 | 1 | RED | A6 | B+ from fuse #4
2 | BLK/WHT | FM1 | LH rear seat heater switch signal | 2 | BLK/WHT | FM300 | LH rear seat heater switch signal
3 | BLK | F1 | Ground to G200 | 3 | BLK | F35 | Ground to G200
4 | BLK/YEL | FB2 | LH rear heater relay ON signal | 4 | BLK/YEL | FB32 | LH rear heater relay ON signal
5 | BRN | X1 | B+ from fuse #15 | 5 | BRN | X33 | B+ from fuse #15
6 | BLK/WHT | FM2 | RH rear seat heater switch signal | 6 | BLK/WHT | FM31 | RH rear seat heater switch signal
7 | BLK/RED | FA2 | RH rear heater relay On signal | 7 | BLK/RED | FA32 | RH rear heater relay ON signal
8-9 | -- | -- | NOT USED | 8-9 | -- | -- | NOT USED

#### Inline Connector C400

Connector Part Information |

• | ZPF 8-1

• | 8 Way F

Connector Part Information

• | ZPM 8-1

• | 8 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | RED/BLU | AP11 | B+ from fuse #18 | A | RED/BLU | AP10 | B+ from fuse #18
B | BLK | F226 | Ground to G103 | B | BLK | F224 | Ground to G103
C | BLU/BLK | PF12 | Fuel gauge signal | C | BLU/BLK | PF11 | Fuel gauge signal
D | BRN/YEL | XB902 | Fuel tank pressure signal | D | BRN/YEL | XB1 | Fuel tank pressure signal
E | BRN/GRN | XU901 | Sensor ground | E | BRN/GRN | XU1 | Sensor ground
F | BLU/BLK | PF901 | 5V reference | F | BLU/BLK | PF1 | 5V reference
G | BLK | F225 | Ground to G400 | G | BLK | F30 | Ground to G400
H | -- | -- | NOT USED | H | -- | -- | NOT USED

#### Inline Connector C401

Connector Part Information |

• | ZFW 6-3

• | 6 Way F

Connector Part Information

• | ZMW 6-3

• | 6 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | GRY/RED | RA1 | RH rear side marker lamp signal | 1 | GRY/RED | RA20 | RH rear side marker lamp signal
2 | GRY/GRN | RU1 | License lamp signal | 2 | GRY/GRN | RU11 | License lamp signal
3 | BLK/GRN | FU1 | RH rear side marker lamp signal | 3 | BLK/GRN | FU30 | RH rear side marker lamp signal
4 | GRY/BLK | RF1 | LH rear side marker lamp signal | 4 | GRY/BLK | RF20 | LH rear side marker lamp signal
5 | BLK | F1 | License lamp signal | 5 | BLK | F44 | License lamp signal
6 | BLK/WHT | FM1 | LH rear side marker lamp signal | 6 | BLK/WHT | FM30 | LH rear side marker lamp signal

#### Inline Connector C405

Connector Part Information |

• | F 9-23

• | 9 Way F

Connector Part Information

• | M 9-23

• | 9 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BLK/RED | FA807 | Rear compartment release signal | 1 | BLK/RED | FA11 | Rear compartment release signal
2 | BLK/YEL | FB15 | Auxiliary brake lamp signal | 2 | BLK/YEL | FB5 | Auxiliary brake lamp signal
3 | GRY/GRN | RU12 | Taillamp (middle) signal | 3 | GRY/BLK | RF1 | Taillamp (middle) signal
4 | BLK | F48 | Ground to G201 | 4 | BLK | F48 | Ground to G201
5 | -- | -- | NOT USED | 5 | -- | -- | NOT USED
6 | BLK/YEL | FB806 | Rear compartment release signal | 6 | BLK/YEL | FB21 | Rear compartment release signal
7 | BRN/BLU | XP901, XP982 | Rear compartment lamp switch signal | 7 | BRN/BLU | XP1 | Rear compartment lamp switch signal
8 | WHT/BLK | MF10 | Transmission position signal | 8 | WHT/BLK | MF10 | Transmission position signal
9 | BRN/WHT | XM9 | Rear compartment lamp switch signal | 9 | BRN/WHT | XM8 | Rear compartment lamp switch signal

#### Inline Connector C500

Connector Part Information |

• | ZFW 40-1

• | 40 Way F

Connector Part Information

• | ZMW 40-1

• | 40 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BLK | F8 | Ground to G200 | 1 | BLK | F1 | Ground to G200
2 | RED | A1 | B+ from fuse #1 | 2 | RED | A2 | B+ from fuse #1
3-4 | -- | -- | NOT USED | 3-4 | -- | -- | NOT USED
5 | GRY | R11 | RH outside rear view mirror signal | 5 | GRY | R11 | RH outside rear view mirror signal
6 | BRN/BLU | XP810 | Driver door lamp signal | 6 | BRN/BLU | XP810 | Driver door lamp signal
7 | BLK/BRN | FX805 | Door lock signal | 7 | BLK/BRN | FX805 | Door lock signal
8-11 | -- | -- | NOT USED | 8-11 | -- | -- | NOT USED
12 | BRN | X999 | B+ from fuse #13 | 12 | BRN | X10 | B+ from fuse #13
13 | BRN/PPL | XY810 | Key disarm signal | 13 | BRN/PPL | XY810 | Key disarm signal
14-15 | -- | -- | NOT USED | 14-15 | -- | -- | NOT USED
16 | BLU/RED | PA2 | Window down signal | 16 | BLU/RED | PA2 | Window down signal
17 | GRY/GRN | RU5 | Window up signal | 17 | GRY/GRN | RU6 | Window up signal
18 | -- | -- | NOT USED | 18 | -- | -- | NOT USED
19 | BLK/WHT | FM10 | B+ from fuse #11 | 19 | BLK/WHT | FM2 , FM15 | B+ from fuse #11
20 | BLU | P1 | Door speaker and tweeter signal | 20 | BLU | P1 | Door speaker and tweeter signal
21 | BLK/RED | FA7 | Outside rear view mirror common | 21 | BLK/RED | FA7 | Outside rear view mirror common
22 | BRN/BLU | XP1 | Door speaker and tweeter signal | 22 | BRN/BLU | XP1 | Door speaker and tweeter signal
23 | YEL | B6 | Door open signal | 23 | YEL | B11 | Door open signal
24 | YEL | B12 | Memory control signal | 24 | YEL | B81 | Memory control signal
25 | BLK/YEL | FB803 | Window actuator signal | 25 | BLK/YEL | FB9 | Window actuator signal
26 | RED/BLU | AP806 | Door lamp signal | 26 | RED/BLU | AP888 | Door lamp signal
27 | BLU | P3 | Memory control signal | 27 | BLU | P3 | Memory control signal
28 | -- | -- | NOT USED | 28 | -- | -- | NOT USED
29 | BLK/PPL | FY805 | Door unlock signal | 29 | BLK/PPL | FY805 | Door unlock signal
30-31 | -- | -- | NOT USED | 30-31 | -- | -- | NOT USED
32 | BLK/BRN | FX60 | Memory potentiometer signal | 32 | BLK/BRN | FX60 | Memory potentiometer signal
33 | BRN | X60 | Memory potentiometer signal | 33 | BRN | X60 | Memory potentiometer signal
34 | BLK/RED | FA809 | Window actuator signal | 34 | BLK/RED | FA809 | Window actuator signal
35 | -- | -- | NOT USED | 35 | -- | -- | NOT USED
36 | GRY | R60 | Memory potentiometer signal | 36 | GRY | R60 | Memory potentiometer signal
37 | GRN | U80 | Memory control signal | 37 | GRN | U100 | Memory control signal
38 | GRY/GRN | RU50 | Memory potentiometer signal | 38 | GRY/GRN | RU60 | Memory potentiometer signal
39 | BRN/YEL | XB42 | Side impact sensor signal | 39 | BRN/YEL | XB42 | Side impact sensor signal
40 | YEL | B41 | Side impact sensor signal | 40 | YEL | B42 | Side impact sensor signal

#### Inline Connector C600

Connector Part Information |

• | ZFW 40-1

• | 40 Way F

Connector Part Information

• | ZMW 40-1

• | 40 Way M

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BLK | F9 | Ground to G200 | 1 | BLK | F1 | Ground to G200
2 | RED | A4 | B+ from fuse #1 | 2 | RED | A2 | B+ from fuse #1
3-4 | -- | -- | NOT USED | 3-4 | -- | -- | NOT USED
5 | GRY | R110 | RH outside rear view mirror signal | 5 | GRY | R4, R5 | RH outside rear view mirror signal
6 | BRN/BLU | XP809 | Passenger door lamp signal | 6 | BRN/BLU | XP810 | Passenger door lamp signal
7 | BLK/BRN | FX804 | Door lock signal | 7 | BLK/BRN | FX805 | Door lock signal
8-15 | -- | -- | NOT USED | 8-15 | -- | -- | NOT USED
16 | BLU/RED | PA1 | Window down signal | 16 | BLU/RED | PA2 | Window down signal
17 | GRY/GRN | RU6 | Window up signal | 17 | GRY/GRN | RU6 | Window up signal
18 | -- | -- | NOT USED | 18 | -- | -- | NOT USED
19 | BLK/WHT | FM22 | B+ from fuse #11 | 19 | BLK/WHT | FM2, FM20 | B+ from fuse #11
20 | YEL | B10 | Door speaker and tweeter signal | 20 | YEL | B1 | Door speaker and tweeter signal
21 | BLK/RED | FA700 | Outside rear view mirror common | 21 | BLK/RED | FA4, FA65 | Outside rear view mirror common
22 | BRN/YEL | XB10 | Door speaker and tweeter signal | 22 | BRN/YEL | XB1 | Door speaker and tweeter signal
23 | YEL | B5 | Door open signal | 23 | YEL | B2 | Door open signal
24 | -- | -- | NOT USED | 24 | -- | -- | NOT USED
25 | BLK/YEL | FB802 | Window actuator signal | 25 | BLK/YEL | FB9 | Window actuator signal
26 | RED/BLU | AP807 | Door lamp signal | 26 | RED/BLU | AP888 | Door lamp signal
27 | BLU | P30 | Memory control signal | 27 | BLU | P2, P10 | Memory control signal
28 | -- | -- | NOT USED | 28 | -- | -- | NOT USED
29 | BLK/PPL | FY804 | Door unlock signal | 29 | BLK/PPL | FY805 | Door unlock signal
30-31 | -- | -- | NOT USED | 30-31 | -- | -- | NOT USED
32 | BLK/BRN | FX65 | Memory potentiometer signal | 32 | BLK/BRN | FX65 | Memory potentiometer signal
33 | BRN | X65 | Memory potentiometer signal | 33 | BRN | X65 | Memory potentiometer signal
34 | BLK/RED | FA802 | Window actuator signal | 34 | BLK/RED | FA809 | Window actuator signal
35 | -- | -- | NOT USED | 35 | -- | -- | NOT USED
36 | GRY | R70 | Memory potentiometer signal | 36 | GRY | R70 | Memory potentiometer signal
37 | -- | -- | NOT USED | 37 | -- | -- | NOT USED
38 | GRY/GRN | RU60 | Memory potentiometer signal | 38 | GRY/GRN | RU60 | Memory potentiometer signal
39 | BRN/WHT | XM430 | Side impact sensor signal | 39 | BRN/WHT | XM42 | Side impact sensor signal
40 | WHT | M44 | Side impact sensor signal | 40 | WHT | M42 | Side impact sensor signal