For 1990-2009 cars

### Removal Procedure

1. Remove the traction control switch cover by gently prying up on the cover.

Important: Mark the position of the traction control switch before removing.

2. Remove the traction control switch from the instrument panel accessary trim panel:

2.1. | Depress both of the locking tabs.

2.2. | Remove the switch from the bezel.

### Installation Procedure

1. Install the traction switch to the instrument panel accessary trim panel.
2. Install the traction control switch cover to the switch.