For 1990-2009 cars

### Removal Procedure

1. Remove hazard switch cover from switch by gently prying on both sides of the cover.

Mark position of the harzard switch before removing the switch from the radio tape player bezel.

2. Depress the tabs on the hazard switch in order to remove the hazard switch from radio tape player bezel.

### Installation Procedure

1. Install the hazard switch to radio tape player bezel.
2. Install the hazard switch cover to switch by gently snapping into place.