For 1990-2009 cars

### Removal Procedure

1. Remove the two bolts from the front bumper guard located in the lower front.
2. Remove the front bumper guard.

### Installation Procedure

1. Hook the front bumper guard to both the fascia and the impact bar to install the front bumper guard.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the front bumper guard bolts.

Tighten
Tighten the front bumper guard bolts to 12 N·m (106 lb in).