For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Caliper Assembly to Steering Knuckle Bolt | 95 N·m + 37 degrees | 70 lb ft + 37 degrees
Engine Mount Nut | 55 N·m | 41 lb ft
Front Crossmember Frame Rear Bolt | 150 N·m + 37 degrees | 111 lb ft + 37 degrees
Front Crossmember Frame Forward Bolt | 65 N·m + 37 degrees | 48 lb ft + 37 degrees
Front Wheel Hub Bearing Nut | 320 N·m | 236 lb ft
Lower Control Arm to Ball Stud Bolt | 35 N·m | 26 lb ft
Lower Control Arm Ball Stud Pinch Bolt | 100 N·m | 74 lb ft
Lower Control Arm Horizontal Bolt | 140 N·m | 103 lb ft
Lower Control Arm Vertical Bolt | 140 N·m | 103 lb ft
Stabilizer Shaft Insulator Bolt | 20 N·m + 37 degrees | 15 lb ft + 37 degrees
Stabilizer Shaft Link Nut | 65 N·m | 48 lb ft
Steering Linkage Outer Tie Rod Nut | 60 N·m + 52 degrees | 66 lb ft + 52 degrees
Strut Assembly to Steering Knuckle Bolt | 70 N·m | 52 lb ft
Strut Assembly Bearing Nut | 55 N·m | 41 lb ft
Strut Assembly Upper Support Nut | 109 N·m | 80 lb ft
Wheel Speed Sensor Bolt | 8 N·m | 71 lb in