For 1990-2009 cars

1. Connect the RH inflatable restraint front side impact module 2-way connector (if equipped with side air bags).
2. Connect the connector position assurance (CPA) to the RH inflatable restraint front side impact module 2-way connector (if equipped with side air bags).
3. Connect the passenger seat belt pretensioner 2-way connector to inline connector C316.
4. Install the RH seat track trim cover.
5. Connect the LH inflatable restraint front side impact module 2-way connector (if equipped with side air bags).
6. Connect the connector position assurance (CPA) to the LH inflatable restraint front side impact module 2-way connector (if equipped with side air bags).
7. Connect the driver seat belt pretensioner 2-way connector to inline connector C315.
8. Install the LH seat track trim cover.
9. Connect the inflatable restraint IP module 2-way connector (1).
10. Connect the connector position assurance (CPA) to the inflatable restraint IP module 2-way connector.
11. Install the inflatable restraint IP module cover. Refer to SIR Module Cover Replacement .
12. Install the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement.
13. Install the upper and lower steering column covers.
14. Staying well away from the inflator modules and the pretensioners, turn the ignition switch to the ON position.

14.1. | The AIR BAG warning lamp will flash seven times.

14.2. | The AIR BAG warning lamp will then turn OFF.

15. Perform the SIR Diagnostic system Check if the AIR BAG warning lamp does not operate as described.