For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle and support. Refer to Lifting and Jacking the Vehicle .
2. Remove the LF tire and wheel assembly. Refer to Wheel Removal .
3. Remove the LF wheelhouse panel:

• | Remove the screws.

• | Remove the nuts.

• | Remove the retainers.

• | Remove the panel.

4. Remove the cooling fan and insulator:

• | Pull forward and downward on the insulator in order to remove.

• | Disconnect the fan from the duct.

• | Disconnect the fan connector.

5. Unclip the duct wiring harness.
6. Unsnap the duct from the engine compartment relay center.

### Installation Procedure

1. Snap the duct into the engine compartment relay center.
2. Clip the duct wiring harness.
3. Install the cooling fan and insulator:

• | Connect the fan connector.

• | Connect the fan to the duct.

• | Push rearward and upward on the insulator in order to install.

4. Install the LH wheel house panel:

• | Install the panel.

• | Install the screws.

• | Install the nuts.

• | Install the retainers.

5. Install the LF tire and wheel assembly. Refer to Wheel Installation .
6. Lower the vehicle.