For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster. Refer to Instrument Cluster Replacement .
2. Remove the voltage-oil pressure gauge module screws from the module.
3. Remove the voltage-oil pressure gauge module from the cluster lens by pulling back the locking tabs and removing.
4. Remove the speedometer-tachometer gauge module screws from the module.
5. Remove the speedometer-tachometer gauge module from the cluster lens by pulling back the locking tabs and removing.
6. Replace the lens.

### Installation Procedure

Important: Snap the locking tabs into position on the module.

1. Install the speedometer-tachometer gauge module to the cluster lens.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the speedometer-tachometer gauge module screws to the module.

Tighten
Tighten the module screws to 1 N·m (9 lb in).

Important: Snap the locking tabs into position on the module.

3. Install the voltage-oil pressure gauge module to the cluster lens.
4. Install the voltage-oil pressure gauge module screws to the module.

Tighten
Tighten the module screws to 1 N·m (9 lb in).

5. Install the instrument cluster. Refer to Instrument Cluster Replacement .