For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Support the transmission using a transmission jack.
3. Remove the transmission crossmember-to-mount nuts (1).
4. Remove the transmission crossmember-to-body bolts (2) and remove crossmember.
5. Remove the transmission mount bolts (1) and mount.

### Installation Procedure

1. Install the transmission mount and bolts (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten
Tighten the bolts to 40 N·m (30 lb ft).

2. Install the transmission crossmember and crossmember-to-body bolts (2).

Tighten
Tighten the bolts to 45 N·m (33 lb ft).

3. Install the crossmember-to-mount nuts (1).

Tighten
Tighten the nuts to 20 N·m (15 lb ft).

4. Remove the transmission jack.
5. Lower the vehicle.