For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 36660-A Torque/Angle Meter

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the engine front crossmember frame. Refer to Front Suspension Crossmember Replacement .
3. Remove the stabilizer shaft insulator bolts.
4. Remove the stabilizer shaft.
5. Remove the insulators from the stabilizer shaft.

### Installation Procedure

1. Install the insulators to the stabilizer shaft.
2. Install the stabilizer shaft.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Important: Use new stabilizer shaft insulator bolts.

3. Use the J 36660-A in order to install the stabilizer shaft insulator bolts.

Tighten
Tighten the stabilizer shaft insulator bolts to 20 N·m (15 lb ft) + 37 degrees.

4. Install the engine front crossmember frame. Refer to Front Suspension Crossmember Replacement .
5. Lower the vehicle.