For 1990-2009 cars

### Removal Procedure

Caution: This vehicle is equipped with a Supplemental Inflatable Restraint (SIR) System. Failure to follow the correct procedure could cause the following conditions:

• | Air bag deployment

• | Personal injury

• | Unnecessary SIR system repairs

In order to avoid the above conditions, observe the following guidelines:

• | Refer to SIR Component Views in order to determine if you are performing service on or near the SIR components or the SIR wiring.

• | If you are performing service on or near the SIR components or the SIR wiring, disable the SIR system. Refer to Disabling the SIR System.

1. Disable the SIR system, if equipped with the inflatable restraint side impact system. Refer to Disabling the SIR System in SIR.
2. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement .
4. Slide the inside door handle forward.
5. Turn the handle downward to disengage from the door.
6. Remove the linkage from the handle.

### Installation Procedure

1. Install the handle linkage.
2. Slide the handle rearward in order to lock into place.
3. Install the water deflector. Refer to Front Side Door Water Deflector Replacement .
4. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
5. Enable the SIR system, if equipped with the inflatable restraint side impact system. Refer to Enabling the SIR System in SIR.