For 1990-2009 cars

1. Install the main case electrical connector (55), if removed.

Notice: Position the wiring harness correctly underneath the transmission oil filter or the electrical wiring harness may be crushed.

2. Install the main case electrical wiring harness (80).
3. Connect the wiring harness to:

• | the Band Control solenoid (323)

• | the 1-2 shift solenoid (303)

• | the 2-3 shift solenoid (307)

• | the case connector (55)