For 1990-2009 cars

Table 1: | Ignition Switch and Lifting Magnet
Table 2: | Inflatable Restraint IP Module
Table 3: | Inflatable Restraint Front Side Impact Module, LH
Table 4: | Inflatable Restraint Front Side Impact Module, RH
Table 5: | Inflatable Restraint Sensing and Diagnostic and Seat Belt Pretensioner Module
Table 6: | Inflatable Restraint Side Impact Sensor (SIS), LH
Table 7: | Inflatable Restraint Side Impact Sensor (SIS), RH
Table 8: | Inflatable Restraint Steering Wheel Module Coil
Table 9: | Passenger Seat Belt Pretensioner

#### Ignition Switch and Lifting Magnet

Connector Part Information |

• | ZF 6-5

• | 5-Way Female (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A905 | B+ from fuse #24
2 | GRN | U900 | Brake to shift signal
U | BRN | X826 | B+ in the ON position
V | BRN | X1 | B+ in the ON or START position
W | RED | A19 | B+ when the key is inserted
Y | RED | A503 | B+ from fuse V2
Z | BLK/RED | FA700 | Starter solenoid signal

#### Inflatable Restraint IP Module

Connector Part Information |

• | ZF 2-16

• | 2-Way Female (YEL)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YEL/BLU | BP10 | Passenger frontal high
2 | YEL/RED | BA10 | Passenger frontal low

#### Inflatable Restraint Front Side Impact Module, LH

Connector Part Information |

• | ZF 2-15

• | 2-Way Female (YEL)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED/YEL | AB11 | Driver side high
2 | BRN/YEL | XB100 | Driver side low

#### Inflatable Restraint Front Side Impact Module, RH

Connector Part Information |

• | ZF 2-15

• | 2-Way Female (YEL)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED/WHT | AM13 | Passenger side high
2 | BRN/WHT | XM14 | Passenger side low

#### Inflatable Restraint Sensing and Diagnostic and Seat Belt Pretensioner Module

Connector Part Information |

• | ZF 45-4

• | 45-Way Female (YEL)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YEL/WHT | BM30 | Driver frontal high
2 | YEL | B30 | Driver frontal low
3 | YEL/RED | BA10 | Passenger frontal low
4 | YEL/BLU | BP10 | Passenger frontal high
5 | BRN | X30 | Ignition feed
6 | BRN/YEL | XB20 | Inflatable restraint indicator
7 | BLK | F108 | Ground to G103
8 | RED/WHT | AM950 | Driver belt high
9 | BRN/WHT | XM950 | Driver belt low
10 | BRN/YEL | XB100 | Driver side low
11 | RED/YEL | AB11 | Driver side high
12 | BRN/WHT | XM10 | Serial data
13 | RED/WHT | AM13 | Passenger side high
14 | BRN/WHT | XM14 | Passenger side low
15 | BRN/YEL | XB950 | Passenger belt low
16-39 | -- | -- | Not used
40 | BRN/PPL | XY999 | ONSTAR signal
41 | YEL | B41 | Driver sensor
42 | BRN/YEL | XB42 | Driver sensor return
43 | BRN/WHT | XM430 | Passenger sensor return
44 | WHT | M44 | Passenger sensor
45 | RED/YEL | AB950 | Passenger belt high

#### Inflatable Restraint Side Impact Sensor (SIS), LH

Connector Part Information |

• | ZFW 2-69

• | 2-Way Female

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YEL | B41, B42 | Driver sensor
2 | BRN/YEL | XB42 | Driver sensor return

#### Inflatable Restraint Side Impact Sensor (SIS), RH

Connector Part Information |

• | ZFW 2-70

• | 2-Way Female

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WHT | M42, M41 | Passenger sensor
2 | BRN/WHT | XM42, XM430 | Passenger sensor return

#### Inflatable Restraint Steering Wheel Module Coil

Connector Part Information |

• | ZF 8-5

• | 8-Way Female (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | F122 | Ground to G201
2 | BRN/WHT | XM1 | Horn relay control signal
3 | RED/WHT | AM116 | LED control signal
4 | BLU/RED | PA101 | Steering wheel switch signal
5-6 | -- | -- | Not used
7 | YEL/WHT | BM 30 | Driver frontal high
8 | YEL | B30 | Driver frontal low

#### Passenger Seat Belt Pretensioner

Connector Part Information |

• | ZF 2-16

• | 2-Way Female (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED/YEL | AB900 | Passenger belt high
2 | BRN/YEL | XB901 | Passenger belt low