For 1990-2009 cars

### Removal Procedure

1. The boot snaps into the console. You can remove the boot by gently pulling on the front end of the boot.

Remove the gear selector boot from the console.

2. Remove the power window switch connector.

Important: Do not pry the switch from the console as damage to the console trim panel may occur.

3. Dislodge the switch from the console by reaching under the console opening near the gear selector.

### Installation Procedure

1. Install the switch into the console by firmly seating the switch with your hand.
2. Install the power window switch connector.
3. Install the gear selector boot to the console by snapping the console into place.